Starter Usage. Buick Roadmaster 1996

For 1990-2009 cars

#### Starter Motor Performance

Application | Specification
--- | ---
4.3L Engine With SD-260
No Load Test at 10 Volts
Current | 51-71 Amps
Pinion Speed | 7000-11000 RPM
Solenoid Windings Test at 10 Volts
Both Windings | 56-80 Amps
Hold-in Windings | 10-20 Amps
5.7L LT1 With PG-250
No Load Test at 10 Volts
Current | 65-90
Starter Drive Pinion Speed | 2700-3200
Solenoid Windings Test at 10 Volts
Both Windings | 60-85 Amps
Hold-in Windings | 10-20 Amps
5.7L LT1 With PG-260
No Load Test at 10 Volts
Current | 64-95 Amps
Starter Drive Pinion Speed | 2825-3275 RPM
Solenoid Windings Test at 10 Volts
Hold-in Windings | 10-20 Amps
Both Windings | 60-85 Amps