SQUEAK AT BASE OF WINDSHIELD (REMOVE 4MM OF MATERIAL). Buick Roadmaster 1994

For 1990-2009 cars

# SQUEAK AT BASE OF WINDSHIELD (REMOVE 4MM OF MATERIAL)

#### SUBJECT: SQUEAK AT BASE OF WINDSHIELD (REMOVE 4MM OF MATERIAL FROM I/P)

#### MODELS: 1994 BUICK ROADMASTER

#### CONDITION:

SOME OWNERS MAY COMMENT ON A SQUEAK AT THE BASE OF THE WINDSHIELD.

#### CORRECTION:

REMOVE 4MM OF MATERIAL FROM THE I/P BY USING THE FOLLOWING PROCEDURE:

1. REMOVE INSTRUMENT PANEL PAD. (REFER TO SERVICE MANUAL PROCEDURE.)

2. CAREFULLY MEASURE 4MM FROM LEADING EDGE (NEXT TO WINDSHIELD) AND MARK A LINE ON THE PANEL. (SEE FIGURE 1.)

3. USING A UTILITY KNIFE, CUT ON MARKED LINE THROUGH FOAM PAD SCORING THE HARD PLASTIC SUBSTRATE. REMOVE CUT FOAM EXPOSING SCORED LINE.

4. USING A SAW TYPE TOOL, CUT ALONG SCORED LINE.

5. REINSTALL INSTRUMENT PANEL PAD AND ANY OTHER PREVIOUSLY REMOVED PARTS.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE: LABOR OPERATION NUMBER: C2510 LABOR TIME: 0.7 HRS. (FOR I/P PAD REMOVAL) ADD: 0.2 HRS. (FOR CUTTING OF I/P PAD)

FIGURES: 1

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.