Vehicle Speed Sensor and Case Extension Removal. Buick Roadmaster 1996

For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 29837 Output Shaft Support Fixture

• | J 38417 Speed Sensor Remover

1. Remove the sensor retaining bolts.
2. In the case of the Y-car, install the J 38417 .
3. Remove the speed sensor and O-ring seal.
4. Remove the case extension bolts.
5. Remove the case extension and the case seal.
6. Remove the output shaft sleeve and the output shaft O-ring seal. Not all models use an output shaft sleeve and O-ring seal.
7. Install the output shaft support fixture.

If the output shaft support fixture is not used, the output shaft may fall free when the input carrier retaining ring is removed.