Fastener Tightening Specifications. Buick Roadmaster 1996

For 1990-2009 cars

Application | N·m | Lb Ft | Lb In.
--- | --- | --- | ---
A/C Compressor Mounting Bolt | 50 | 37 | --
A/C Compressor Mounting Stud | 50 | 37 | --
A/C Compressor Rear Bracket Nut | 41 | 30 | --
Battery Hold Down Retainer Bolt | 18 | 13 | --
Battery Tray Bolt | 25 | 18 | --
Distributor Bolt | 12 | -- | 106
Distributor Cap Bolt | 2.8 | -- | 25
Distributor Rotor Bolt | 0.7 | -- | 6
Drive Belt Tensioner Bolt | 25 | 18 | --
Engine Ground Cable | 30 | 22 | --
Engine-to-Battery Negative Cable Bolt | 4 | -- | 35
Engine Wiring Harness Generator Lead Nut | 13 | -- | 115
Engine Wiring Harness Junction Block-to-Battery Positive Cable Bolt | 6 | -- | 53
Flywheel Inspection Cover Bolts | 15 | 11 | --
Front Wheelhouse Panel Bolt | 25 | 18 | --
Generator and Power Steering Pump Bracket Bolt | 41 | 30 | --
Generator Battery Terminal Nut (CS-130) | 8 | -- | 71
Generator Battery Terminal Nut (CS-144) | 12 | -- | 106
Generator Front Brace Stud Nut | 34 | 25 | --
Generator Mounting Bolt | 50 | 37 | --
Generator Rear Brace Bolt (CS-130) | 25 | 18 | --
Generator Rear Brace Bolt (CS-144) | 50 | 37 | --
Generator Rear Brace Nut | 41 | 30 | --
Generator Rear Bracket Nut | 50 | 37 | --
Generator Rotor Shaft Drive End Nut | 100 | 75 | --
Heater Hose Clip Bolt | 1.9 | -- | 17
Ignition Coil Bolt | 25 | 18 | --
Ignition Coil Stud | 25 | 18 | --
Ignition Coil Module Bolt | 1.7 | -- | 15
Negative Battery Cable Bolt at the Battery | 17 | 13 | --
Negative Battery Cable Ground Bolt | 4 | -- | 35
Negative Battery Cable Nut | 34 | 25 | --
Positive Battery Cable at the Battery | 17 | 13 | --
Positive Battery Cable Bolt | 4.8 | -- | 42
Positive Booster Cable Bolt at Multifuse Relay Center | 20 | 15 | --
Radiator Outlet Hose Support Nut | 20 | 15 | --
Replacement Ignition Coil-to-Bracket Bolt | 2.8 | -- | 25
Solenoid Battery Terminal Nut | 10 | -- | 89
Solenoid Screw | 6.5 | -- | 60
Solenoid Switch BAT Terminal Inner and Outer Nuts | 9 | -- | 80
Solenoid Switch Clamp Bolt | 11 | -- | 97
Solenoid Switch M Terminal Inner Nut | 9 | -- | 80
Solenoid Switch Outer Nut (PG-250) | 8 | -- | 71
Solenoid Switch S Terminal Nut | 2.5 | -- | 22
Spark Plug (With Head Replacement) | 30 | 22 | --
Spark Plug (With Existing Engine Assembly) | 20 | 15 | --
Starter Motor Bolt | 47 | 35 | --
Starter Motor Brush Holder Attachment Bolt (PG-250) | 6.5 | -- | 58
Starter Motor Commutator End Frame Bolt | 8.5 | -- | 75
Starter Motor Heat Shield Nut | 8 | -- | 71
Starter Solenoid Switch-to-Battery Positive Cable Nut | 10 | -- | 89
Starter Through-Bolt (PG-250) | 8.5 | -- | 75
Storage Battery Side Terminal Adapters | 15 | 12 | --
Wire Harness Support Bolt | 40 | 30 | --
Wire Harness Support Channel Bolt (Right) | 12 | -- | 106
Wire Harness Support Channel Bolt (Left) | 12 | -- | 106