IMPACT STRIP LOOSE/MISSING FROM BODY MLDG.-REPAIR/REPLACE. Buick Roadmaster 1992

For 1990-2009 cars

# IMPACT STRIP LOOSE/MISSING FROM BODY MLDG.-REPAIR/REPLACE

#### SUBJECT: IMPACT STRIP LOOSE OR MISSING FROM BODY SIDE MOULDING (REINSTALL OR REPLACE STRIP)

#### VEHICLES AFFECTED: 1991-93 BUICK ROADMASTER "B"-MODELS

THIS BULLETIN SUPERSEDES AND REPLACES CORPORATE BULLETIN REFERENCE NUMBER 231035.** THIS BULLETIN IS BEING REVISED TO ADD 1993 MODEL YEAR

#### Application:

----------- 1991-93 Buick Roadmaster Estate Wagon 1992-93 Buick Roadmaster Sedan

#### CONDITION:

--------- Impact strip loose or missing.

#### CAUSE:

----- Impact strip not properly installed.

#### CORRECTION:

---------- Reinstall impact strip if loose. If impact strip is missing, replace entire moulting assembly per Service Manual procedures in Sections 10-5 Front Fender, 10-6 Doors, 10-7 Rear Quarter and 10-8 Rear End.

Reinstall the impact strip per the following instructions:

#### REMOVE IMPACT STRIP

1. For ease of removal, heat moulting using a heat gun 152 mm (6") from the surface. Apply heat using a circular motion for about 30 seconds. Gradually pull impact strip away from the bright moulding. Avoid bending the impact strip.

2. Lay impact strip, adhesive side up, on a table with a shop cloth to protect the outer surface from scratches.

#### REMOVE ORIGINAL ADHESIVE TAPE

1. Clean the back of the impact strip moulting with oil-free naphtha or alcohol. Allow cleaner to soak in and then use a scraper to remove any adhesive tape. If adhesive cleaners such as *3M General Purpose Adhesive Cleaner #08984 are used, do not saturate the impact strip with these as this could hinder adhesion of the new acrylic foam tape.

2. Use oil-free naphtha, alcohol or 3M General Purpose Adhesive Cleaner #08984 to clean bright moulding. Follow manufacturer's directions for use. Allow to soak in and then use a scraper to remove any adhesive- tape. Be careful not to scrape the portion of bright moulting that will be exposed after the impact strip is installed.

#### OPTIONAL:

-------- Use 3M Scotch-Brite Moulting Adhesive and Stripe Removal Disk 3M #07501 and Roloc & Holder 3M #7500 to remove original adhesive tape. Attach the assembled 3M parts to a drill capable of a speed of 4000 RPM. Carefully remove the original adhesive tape from the impact strip and the bright moulting. Wipe impact strip and bright moulting with oil-free naphtha or alcohol to remove any residue.

#### REINSTALL IMPACT STRIP

1. Apply 3M acrylic foam tape #06381 to the impact strip along the length across the top, 2.0 mm (1/16") down from the top edge.

2. Press firmly (wallpaper seam roller, screwdriver handle, thumb, etc.) along the release liner length from the center and work toward the ends and cut any access from the ends.

3. To ensure a good bond, the bright moulting temperature should be 70 degrees Fahrenheit (21 degrees Celsius).

4. Remove 152 mm (6") of the release liner and apply the impact strip to the bright moulting, aligning the forward edge first. Continue removing the release liner and applying the impact strip to the bright moulding.

#### NOTICE: Prior to Step 5, cover impact strip or rolling device with a shop cloth to prevent damage to exposed surface of impact strip.

5. Beginning at the forward edge, press firmly (wallpaper seam roller, screwdriver handle, can, etc.) several times over the impact strip.

For vehicles repaired under warranty use:

Labour Time: 0.8 HR one moulding 0.7 HR each additional

Time includes replacement of tape and reinstallation of existing impact strip.

We believe this source and their equipment to be reliable. There may be additional manufacturers of such equipment. General Motors does not endorse, indicate any preference for or assume any responsibility for the product or equipment for these firms or for any such items which may be available from other sources.

LABOUR OPERATION: Use published allowances and labour times for replacement of complete moulding assemblies.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.