DRIVE AXLE TRI-POT SEAL CLAMP PART NUMBERS. Buick Skyhawk 1986

For 1990-2009 cars

# DRIVE AXLE TRI-POT SEAL CLAMP PART NUMBERS

#### MODELS AFFECTED: 1986 NON TURBO SKYHAWKS

For the 1986 model year, a limited quantity of non turbo Skyhawk vehicles, with both automatic and manual transaxles, have been built using a low-profile, earless Tri-Pot seal retaining clamp on the left-hand inboard axle joint.

These assemblies may be serviced with Seal Service Kit Tri-Pot 7845350 (which contains standard clamp 7843226), using J35910 Drive Axle Seal Clamp Pliers. Refer to Illustration.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.