REAR CONTROL ARM BUSHING REPLACEMENT PROCEDURE. Buick Skyhawk 1985

For 1990-2009 cars

# REAR CONTROL ARM BUSHING REPLACEMENT PROCEDURE

#### Models Affected: All Skyhawks and Somerset Regals

#### NOTE: This bulletin is being reissued to correct the bulletin number and put it in its correct filing section. Please discard Bulletin 85-9-12 with file number 85-251-3 and replace it with this one.

The rear control arm bushing replacement procedure on page 3D1-15 of the 1985 Buick Chassis Service Manual does not clearly show the Special "J" tools installed. The following illustration shows the tool installation and should be refered to when replacing bushings.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.