PANEL DISTORTION FRONT END. Buick Skyhawk 1982

For 1990-2009 cars

# PANEL DISTORTION FRONT END

#### MODELS AFFECTED: 1982 Skyhawk

The front end panel on 1982 Skyhawk models may distort away from its retainers above the headlamps. Retainers have been released to hold the front end panel in place. These retainers may be obtained through WDDGM by ordering the following part numbers:

Right Side - 22520274

Left Side - 22520275

The retainers can be installed by using the following procedure:

1. Remove headlight bezel.

2. Remove Parking Lamp Assembly.

3. Install front end panel retainer between fascia and existing support panel so that the bolt hole lines up with mounting hole for parking lamp assembly. (See Illustration).

Proper retainer is indicated with a letter stamped on top. L for Left, R for Right. See inset, Illustration.

4. Install parking lamp assembly and position so that top mounting bolt goes through retainer, then through lamp assembly.

5. Install headlamp bezel.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.