SQUEAK IN STEERING WHEEL HORN SHROUD REVISION. Buick Skyhawk 1982

For 1990-2009 cars

# SQUEAK IN STEERING WHEEL HORN SHROUD REVISION

#### MODELS AFFECTED: 1982 Skyhawks

Some subject models may have a squeaking or creaking noise at the ends of the horn shroud when the steering wheel is flexed. Urethane foam is being added to the horn shroud in production to eliminate this noise.

If an owner's vehicle requires correction of this noise, remove horn pad and add urethane foam as instructed on Page 2 of this bulletin.

WARRANTY INFORMATION

Operation Number T5044

Labor Time 0.2 Hour

Trouble Code 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.