Technical Service Bulletins Buick Skyhawk 1988

For 1990-2009 cars

# Technical Service Bulletins

- 2008-06-04: No Movement When Transmission is Shifted to Drive or Third - Normal Operation When Shifted to Second, First or Reverse (Replace Forward Sprag Assembly) (08-07-30-027)
- 2007-12-05: 60 Degree V6 Engine Oil Leak at Crankshaft Front Oil Seal (Use New Crankshaft Front Oil Seal Installer Tool EN-48869) (07-06-01-023)
- 2007-10-02: Engine Oil Leak at Crankshaft Rear Main Oil Seal (Install Revised Crankshaft Rear Main Oil Seal Using Revised Rear Main Seal Installer and Remover Tools) (05-06-01-019F)
- 2006-01-27: Service VME - Use Correct Engine Oil Drain Plug - keywords drain engine leak oil pan plug replace (PIP3696)
- 2006-01-18: Info - New Product Feedback Form and Process for Automatic Transmission Core Returns (01-07-30-029A)
- 2004-03-18: No TCC Apply , MIL On , TCC Surge , Possible P0740 , P1870 , or 39 after Installation of Reman ( SRTA ) 4T60 / 4T60E - kw case cover converter slip transmission (PI01880A)
- 2001-04-06: Info - Current CIPS Campaign Number to Previous DIvisional Campaign Number (01-00-89-008)
- 2001-03-02: Info - February, 2001 Bulletin Summary (01-00-89-006)
- 2000-04-05: Snow Intrusion Into Rr Drum Brake Assem (Replace Rr Brake Assem Backing Plates) (00-05-24-001)
- 1999-12-23: Info - Dealer Installed Rear Seat Lap/Shoulder Belt Kits (99-09-40-006)
- 1998-06-03: INFO - NEW TOOL J-42958, REV. CHARTS AND SCHEM. FOR CRUISE (83-90-08)
- 1998-03-10: INFO. NEW TOOL J-41450-B RELEASED FOR CS GEN DIAG. (83-64-09)
- 1998-01-12: INFO. FRONT. SUPP. INFLAT. RESTRAINTS (SIR) ON-OFF SWITCH (73-90-23)
- 1997-12-11: WARRANTY ADMIN - ACDELCO REMANUFACTURED ENGINES (72-05-07)
- 1997-11-20: CLARIFICATION OF RAIL DUST REM (A5575-A5580) (72-05-11)
- 1997-11-01: WARRANTY ADMIN. - LABOR OPERATION CODE Z1241 (62-05-02A)
- 1997-09-01: INFO. ON ALUMINUM HEATER CORE AND/OR RADIATOR REPL. (73-62-13A)
- 1997-05-29: INFO ON AUTO TRANS OIL COOLER FLUSHING &FLOW CHECK PROC. (77-71-59)
- 1997-05-12: INFORMATION -TWO PART URETHANE ADHESIVE (73-10-54)
- 1997-04-17: INFO. ON A/C TOOL AND EQUIPMENT MAINTENANCE (63-12-08A)
- 1997-02-07: SERVICE ISSUES FOR VEHICLES WITH R12 OR R134A A/C SYSTEMS (73-12-04)
- 1997-01-31: INFO. NEW BODY SEALER TAPE FOR COLLISION REPAIRS (73-10-49)
- 1997-01-13: INFO. ON COMPACT DISC PLAYERS- PROCEDURES (64-96-01)
- 1997-01-01: GUIDELINES FOR RETROFITTING R-12 VEH. TO R-134A (43-12-07E)
- 1996-12-01: SERVICE ADMINISTRATION - WARRANTY CLAIMS PROCESSING (31-05-03C)
- 1996-11-15: INFO. REFERENCE CHART FOR A/C COMPRESSOR SEAL WASHERS (63-12-15)
- 1996-10-15: INFO. ON THE GENERAL MOTORS KEY CODE VOICE RESPONSE SYSTEM (61-01-11)
- 1996-10-01: PROCEDURE TO HANDLE CUSTOMER RADIO CONCERNS (68-96-01A)
- 1996-09-01: ACDELCO SERVICE CENTER LOC. FOR ODOMETER/SPEEDOMETER (66-83-04A)
- 1996-06-05: WARRANTY ADMIN. - GOODWRENCH SERVICE PLUS LIFETIME SERVICE (68-05-03)
- 1996-05-10: INFO. ON SERVICE ISSUES FOR VEHICLES WITH R12 OR R134A (63-12-09)
- 1996-05-07: INFORMATION ON CAMPAIGN SYSTEM COMMONIZATION (62-07-01)
- 1996-05-06: INFO. ON ENHANCED EMISSION INSPECTION MAINTENANCE PROGRAM (63-65-32)
- 1996-05-01: AC DELCO LOCATOR SVCS FOR DELCO ELECTRONICS EXCHANGE (58-83-02B)
- 1996-05-01: WARRANTY ADMINISTRATION TIRE REPLACEMENTS (60-05-01A)
- 1996-04-15: INFO. ON HEADLAMP LENS DISTORTION (63-81-11)
- 1996-02-02: INFORMATION ON UPDATED BATTERY REPLACEMENT CATALOG NUMBERS (63-64-01)
- 1996-01-04: TECHNICAL ASSISTANCE PRE-CALL WORKSHEET (51-01-07)
- 1995-12-11: SMU - SECTION 6A - ENGINE MECHANICAL (57-61-37)
- 1995-11-29: INFO. ON ENHANCED EMISSION INSPECTION MAINTENANCE (53-65-07)
- 1995-10-10: WARRANTY INFORMATION ALL MODELS - ALL YEARS (58-05-03)
- 1995-10-09: INFO. ON DAYTIME RUNNING LAMPS (DRL) (53-82-09)
- 1995-09-01: WARRANTY INFORMATION - LABOR TIME SUBMISSION FORMAT (58-05-01A)
- 1995-09-01: REPLACEMENT OF ISOLATION DIODES (93-8-20)
- 1995-08-10: REVISED TECH 1 MASS STORAGE CARTRIDGE (MSC) OXYGEN SENSOR (51-65-47)
- 1995-06-12: INFO. ON REFORMULATED GASOLINE (RFG) (57-01-02)
- 1995-06-01: CAMPAIGN: SERVICE PART FUEL TANK SENDER RING WELDS (91-C-51)
- 1995-05-23: WARRANTY ADMINISTRATION WARRANTY INFORMATION (57-05-02)
- 1995-05-15: INFORMATION ON CONTAMINATED R12 REFRIGERANT TESTING (53-12-05)
- 1995-04-27: INFORMATION ON GM CAMPAIGN IDENTIFICATION LABEL (51-01-03)
- 1995-04-01: INFORMATION ON SIERRA-BRAND ENGINE COOLANT (43-62-01B)
- 1995-03-28: WARRANTY ADMINISTRATION DEALER/RETAILER ADMINISTRATION (57-05-01)
- 1995-03-01: SMU - SECTION 0 - GENERAL INFORMATION (57-02-01)
- 1995-02-21: SMU - SECTION 6A - REVISED BALANCE SHAFT (57-61-07)
- 1995-02-03: SMU - INFO. ON INSPECTION/ MAINTENANCE (I/M) EMISSIONS (51-65-02)
- 1995-01-11: ENHANCED EMISSION INSPECTION MAINTENANCE PROGRAM (43-65-10)
- 1995-01-04: SMU - SECTION 6E2, 6E3 - DRIVABILITY & EMISSIONS (41-65-32)
- 1994-11-29: INFO. ON ENHANCED EMISSION INSPECTION MAINTENANCE PROGRAM (43-65-07)
- 1994-11-23: FRONT BRAKE PULSATION - 'NEW' DIAGNOSIS (43-50-09)
- 1994-10-25: REV. TO ADHESIVE CAULKING KIT, NEW PRIMERS & PART NUMBERS (43-10-48)
- 1994-09-15: DLR. PRODUCT CAMPAIGN BULLETIN NUMBERING SYSTEM (41-01-03)
- 1994-09-12: INFO. ON NEW PROM/MEMCAL IDENTIFICATION MARKINGS (44-65-01)
- 1994-09-08: CONTAMINATED A/C REFRIGERANT (INFORMATIONAL) (43-12-23)
- 1994-09-01: INFORMATION ANNOUNCING THE NEW CORPORATE BULLETIN (33-01-05A)
- 1994-08-16: OBTAINING TECHNICAL ASSISTANCE (I/M 240 REPAIRS) (43-65-06)
- 1994-08-03: WARRANTY ADMINISTRATION-NEW WARRANTY CLAIM PROCESSING SYS. (41-05-02)
- 1994-07-18: INFORMATION ON RELEASE OF SERVICE PKG. FOR NICKEL TAPE (14-93-01)
- 1994-06-30: INFORMATION ON J39400 A/C LEAK DETECTOR MAINTENANCE KIT (43-12-18A)
- 1994-06-20: INFORMATION ON SPEED RATED TIRES (43-35-02)
- 1994-06-08: WARRANTY ADMINISTRATION - NEW LABOR OPERATION NUMBER (42-05-06)
- 1994-05-13: WARRANTY ADMINISTRATION - EMISSION WARR. PARTS COVERAGE (47-05-01)
- 1994-05-01: INFO. ON VEHICLES EQUIPPED WITH A WEBASTO SUNROOF (43-10-18A)
- 1994-04-08: REDUCED PWR STEERING ASSIST AT LOW AMBIENT TEMPERATURES (03-32-06)
- 1994-03-29: ENHANCED INSPECTION MAINTENANCE PROGRAMS (43-65-05)
- 1994-02-15: INFORMATION ON TRANSAXLE OIL FILTER DIFFERENCES (47-71-03)
- 1994-02-01: INFORMATION ON AFTER MARKET ANTI-LOCK BRAKE SYS. PRODUCTS (43-50-01)
- 1993-12-22: RETROFITTING R-12 VEHICLES TO R-134A (INFORMATIONAL) (33-12-26)
- 1993-10-22: CLEARCOAT DEGRADATION-CHALKING & WHITENING (REPAIR PROCEDURE) (33-17-08)
- 1993-08-01: TIRES SLIPPING ON WHEELS USE PROPER TIRE MOUNTING PROC (93-3-6)
- 1993-08-01: INFO. ON COSMETIC DAMAGE TO ALUMINUM WHEELS DURING BALANC. (93-3-10)
- 1993-08-01: TIRES SLIPPING ON WHEELS USE PROPER TIRE MOUNTING PROC (93-3E-103)
- 1993-08-01: INFO. ON COSMETIC DAMAGE TO ALUMINUM WHEELS DURING BALANC. (93-3E-104)
- 1993-07-01: LEAKING CAST ALUMINUM WHEELS (REPAIR WITH ADHESIVE SEALANT) (93-3-14)
- 1993-05-25: RECYCLING OF USED OIL FILTERS (INFORMATIONAL) (93-0-6)
- 1993-05-19: INFO. ON SERVICING VEHICLE WITH CONTAMINATED TRANS. FLUID (93-7-1)
- 1993-05-19: INFO. ON SERVICING VEHICLE WITH CONTAMINATED TRANS. FLUID (93-7A-142)
- 1993-05-06: A/C R-134A REFRIGERANT (INFORMATION) (93-1-9)
- 1993-05-06: A/C R-134A REFRIGERANT (INFORMATION) (93-1B-126)
- 1993-04-30: WINDSHIELD WIPER CHATTER AND WIPEABILITY (93-8C-116)
- 1993-04-30: BINDING/STICKING LOCK CYLINDER RECOMMENDED LUBRICATIONS (93-10-194)
- 1993-03-16: ILLUSTRATED STEERING SYSTEM BLEED PROCEDURE (38-30-01A)
- 1993-01-27: INFO. ON FACTORS THAT AFFECT FUEL ECONOMY (30-65-02)
- 1993-01-21: SERVICE MANUAL UPDATE-SEC.10-8 REAR COMP LID HINGE TORQUE ROD (89-10-39)
- 1993-01-21: SERVICE MANUAL UPDATE-SEC.10-8 REAR COMP LID HINGE TORQUE ROD (93-10-606)
- 1992-12-01: ENG. MISS, HESITATION & ROUGH PIERCED SECONDARY IGNITION (93-6D-102)
- 1992-11-30: SERVICE GUILD: INFO. ON THE EFFECT OF FUEL VOLATILITY (92-6E-23)
- 1992-11-30: SERVICE GUILD: INFO. ON THE EFFECT OF FUEL VOLATILITY (93-6C-100)
- 1992-11-30: ALTERNATE REFRIGERANTS INFORMATION (93-1B-102)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-7)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (92-2-128)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-179)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-148)
- 1992-10-31: A/C COMPRESSOR SHAFT NUT REMOVAL (IMPROVED QUALITY) (93-1D-100)
- 1992-08-03: ALTERNATE REFRIGERANTS INFORMATION (92-1-16)
- 1992-06-16: SERVICE GUILD: INFO ON AVOID DAMAGE TO TIRE WHEELS (92-3-17)
- 1992-06-16: SERVICE GUILD: INFO ON AVOID DAMAGE TO TIRE WHEELS (92-3-123)
- 1992-06-02: SLIPS IN LOW/REVERSE NO REVERSE-REPLACE LOW CLUTCH (92-73T40-1)
- 1992-06-02: SLIPS IN LOW/REVERSE NO REVERSE-REPLACE LOW CLUTCH (92-73T40-100)
- 1992-05-31: BRAKE PULSATION SERVICE INFORMATION (88-5-121)
- 1992-05-27: A/C LEAK (DIAGNOSIS BULLETIN) ALL MODELS 1992 AND PRIOR (92-1-13)
- 1992-04-01: PROM I.D. NOT RECOGNIZED BY THE T-100 (GM CAMS) TERMINAL (23-65-08)
- 1992-03-25: TECH-1 GM 88-92 BRAKE CARTRIDGE EXCHANGE PROGRAM (92-1-12)
- 1992-03-24: INFO ON COATED WHEEL WEIGHTS USED FOR ALUMINUM WHEELS (92-3-12)
- 1992-03-24: INFO ON COATED WHEEL WEIGHTS USED FOR ALUMINUM WHEELS (92-3-121)
- 1992-02-05: CRUISE CONTROL DROPOUT (FAILS TO SET OR RESUME) (92-9-9)
- 1992-02-05: CRUISE CONTROL DROPOUT (FAILS TO SET OR RESUME) (92-8-140)
- 1992-01-31: A/C R-12 CHARGING CAPACITY (CHART) (92-1-109)
- 1992-01-09: SIR SENSOR REPLACE POLICY REV. ALL 1988-92 CARS WITH SIR (92-9-8)
- 1992-01-09: SIR SENSOR REPLACE POLICY REV. ALL 1988-92 CARS WITH SIR (92-8-127)
- 1991-12-14: LEAD/PULL TORQUE/MEMORY STEER, STEERING WHEEL OFF CENTER (92-3-110)
- 1991-11-15: A/C R-12 CHARGING CAPACITY CADILLAC CHARGING TABLE (92-8-112)
- 1991-11-06: BINDING/STICKING LOCK CYLINDER RECOMMENDED LUBRICATIONS (92-10-20)
- 1991-11-06: BINDING/STICKING LOCK CYLINDER RECOMMENDED LUBRICATIONS (92-2-141)
- 1991-10-15: A/C COMPRESSOR SHAFT NUT REMOVAL (IMPROVED QUALITY) (93-1-2)
- 1991-10-11: A/C COMPRESSOR SEALING WASHER USAGE (NEW DESIGN) (92-1-3)
- 1991-10-11: A/C COMPRESSOR SEALING WASHER USAGE (NEW DESIGN) (92-1-103)
- 1991-10-02: DEXRON IIE A/T FLUID PREFERRED (GENERAL INFORMATION) (92-7-2)
- 1991-10-02: DEXRON IIE A/T FLUID PREFERRED (GENERAL INFORMATION) (92-7-100)
- 1991-09-30: 3-4 CLUTCH/2-4 BAND SERVICE INFORMATION/SERVICE PROCEDURES (91-7-113)
- 1991-09-17: SQUAWK/CLUNK NOISE FROM FRT. SUSP.-REPLACE STABILIZER BUSH. (91-3-20)
- 1991-09-17: SQUAWK/CLUNK NOISE FROM FRT. SUSP.-REPLACE STABILIZER BUSH. (91-3-132)
- 1991-08-09: CELLULAR TELEPHONE PROGRAM (DELCO ELECT.) NEW INFORMATION (92-9-4)
- 1991-08-08: SERVICE GUILD: EVALUATING PEENED SPACER PLATE (91-7-3)
- 1991-08-08: SERVICE GUILD: EVALUATING PEENED SPACER PLATE (91-7-115)
- 1991-07-31: WINDSHIELD WIPER BLADE CHATTER (REVISED BLADE & INSERT) (91-2-234)
- 1991-07-24: DAMAGED ECM/PCM MIS-DIAGNOSIS INCORRECT 'TAP-TESTING' (92-6E-3)
- 1991-07-24: DAMAGED ECM/PCM MIS-DIAGNOSIS INCORRECT 'TAP-TESTING' (91-6-121)
- 1991-06-21: WINDSHIELD WIPER CHATTER (REVISED BLADE & INSERTS) (89-10-38)
- 1991-06-21: WINDSHIELD WIPER CHATTER (REVISED BLADE & INSERTS) (91-8-223)
- 1991-06-20: DISPOSAL OF LIVE (UNDEPLOYED) SIR INFLATOR MODULES (92-9-2)
- 1991-06-13: RETAINING MEMORIES IN ELECT. DEVICES WITH BAT. DISCONNECTED (91-8-212)
- 1991-05-15: BINDING OR INOP REVERSE STUCK 3-4 SEQ. VALVE 2-3 SHIFT (91-74L60-104)
- 1991-04-30: A/C REFRIGERANT LOSS DUE TO LOOSE/MISSING ACCESS CAPS (91-1-4)
- 1991-04-30: A/C REFRIGERANT LOSS DUE TO LOOSE/MISS. ACCESS FITTING CAP (91-1-123)
- 1991-04-19: DAMAGE TO ECM/PCM CIRCUIT BOARD WHEN INSTALLING MEM-CAL (91-6E-18)
- 1991-04-19: DAMAGE TO ECM/PCM CIRCUIT BOARD WHEN INSTALLING MEM-CAL (91-6-117)
- 1991-04-15: CLEANING OF UPPER I/P SURFACES CLEANING PROCEDURES (91-0-5)
- 1991-04-15: CLEANING OF UPPER I/P SURFACES CLEANING PROCEDURES (91-2-197)
- 1991-03-04: SER.MANUAL UPDATE SEC.8A,B & C DELETION OF FLASH TO PASS FUSE (91-8-182)
- 1991-02-28: WINDSHIELD WIPER CHATTER AND WIPEABILITY (91-2-149)
- 1991-02-28: TIRE DAMAGE CAUSED IN GM ASSY. PLANTS-REPLACEMENT PROCEDURES (91-3-115)
- 1991-02-25: CLUNK FROM ENGINE COMPARTMENT WHEN TURNING & LOOSE STEERING (90-3-20)
- 1991-02-25: CLUNK FROM ENGINE COMPARTMENT WHEN TURNING & LOOSE STEERING (90-3-141)
- 1991-02-15: NO START/VEHICLE BATTERY DEAD PARASITIC CURRENT DRAIN TEST (91-6D-5)
- 1991-02-15: INFO ON MULTEC FUEL INJECTORS DO NOT CLEAN MULTEC INJECTORS (91-6-111)
- 1991-02-15: NO START/VEHICLE BATTERY DEAD PARASITIC CURRENT DRAIN TEST (91-8-172)
- 1991-01-23: NEW DEPARTURE HYATT ROLLER CLUTCH ALL HYDRA-MATIC 3T40 (91-73T40-4)
- 1991-01-23: NEW DEPARTURE HYATT ROLLER CLUTCH ALL HYDRA-MATIC 3T40 (91-73T40-103)
- 1991-01-15: WINDSHIELD WIPER CHATTER AND WIPEABILITY SERVICE PROCEDURE (89-10-37)
- 1991-01-15: WINDSHIELD WIPER CHATTER AND WIPEABILITY SERVICE PROCEDURE (90-2-258)
- 1991-01-15: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (91-73T40-101)
- 1991-01-15: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (91-74T60105)
- 1991-01-15: SERVICE MAN. UPDATE SEC. 6E2 DRIVEABILITY & EMISSION REV. (88-6E-32A)
- 1991-01-02: NEW TWILIGHT SENTINEL MODULE SERVICE PART AND INFO (89-8-33)
- 1991-01-02: NEW TWILIGHT SENTINEL MODULE SERVICE PART AND INFO (91-8-146)
- 1990-12-31: CHATTERING WIPER BLADES OR WIPEABILITY (91-0-4)
- 1990-12-31: CHATTERING WIPER BLADES OR WIPEABILITY (91-2-123)
- 1990-12-31: BRAKE EFFECTIVENESS AFTER ROTOR REFINISHING (91-5-109)
- 1990-12-15: NEW PLATES-4TH CLUTCH REACTION FORWARD CLUTCH/LOW & REV. (90-74T60-122)
- 1990-12-15: GRINDING OR GROWLING NOISE IN PARK ON INCLINE (90-74T60121)
- 1990-11-15: FAILURE TO RUN COLD OFR HES. NEW CAL-PROM LISTING (90-620-101)
- 1990-11-14: SERV MAN UPDT-SEC.6A1,6C,6E2 FUEL PRESSURE RELIEF (88-6E-34)
- 1990-11-14: SERV MAN UPDT-SEC.6A1,6C,6E2 FUEL PRESSURE RELIEF (91-620-100)
- 1990-11-14: SERVICE MANUAL UPDATE-SEC.6E2 FUEL SYSTEM DIAGNOSIS-REVISED (91-620-101)
- 1990-09-30: (SRTA) MODEL UPDATE WITH 3T40 (125C) (91-7125-1)
- 1990-09-21: NEW FORWARD CLUTCH LO & REV. WAVED PLATES (91-7-1)
- 1990-09-21: NEW FORWARD CLUTCH LO & REV. WAVED PLATES (91-74T60-106)
- 1990-09-13: NEW SILICONE BEADED SIDE COVER & BOTTOM PAN GASKET (91-7125-3)
- 1990-09-13: NEW SILICONE BEADED SIDE COVER & BOTTOM PAN GASKET (91-73T40-100)
- 1990-08-15: STATE EMISSIONS TESTING INFORMATION / PROCEDURE (91-6E-2)
- 1990-08-02: NEW WARRANTY CLAIM FAILURE CODES (90-0-10)
- 1990-07-26: RELEASE OF ANTENNA BEZEL NUT-1991 ESSENTIAL TOOL (91-9-3)
- 1990-07-24: BRAKE EFFECTIVENESS CHANGE AFTER ROTOR & BRAKE PAD WORK (90-5-12)
- 1990-07-09: DASH PAD WARPED AT DEFROSTER DUCT (90-10-25)
- 1990-06-29: COATED WHEEL WEIGHTS FOR ALUMINUM WHEELS (91-3-1)
- 1990-06-29: COATED WHEEL WEIGHTS FOR ALUMINUM WHEELS (90-3-127)
- 1990-06-22: BRAKE ROTOR REFINISH PARTS ORDERING INFORMATION (90-5-10)
- 1990-06-22: BRAKE ROTOR REFINISH PARTS ORDERING INFORMATION (90-5-118)
- 1990-05-18: DASH PAD WARPED AT DEFROSTER DUCT (90-2-175)
- 1990-04-26: SQUAWK NOISE FROM THE REAR NEW SPRING UPPER INSULATOR (90-3-13)
- 1990-04-26: SQUAWK NOISE FROM THE REAR NEW SPRING UPPER INSULATOR (90-3-121)
- 1990-04-24: HIGH OIL CONSUMPTION CONCERN CORRECTIVE SERVICE PROCEDURE (89-6-23)
- 1990-04-24: HIGH OIL CONSUMPTION CONCERN CORRECTIVE SERVICE PROCEDURE (90-620-100)
- 1990-04-11: INSTALLATION GUIDELINES FOR AFTERMARKET ACCESSORIES (91-9-1)
- 1990-04-11: INSTALLATION GUIDELINES FOR AFTERMARKET ACCESSORIES (90-8-184)
- 1990-04-06: SHIFTABILITY CONCERNS ON 5-SPEED MANUAL TRANSAXLE (89-7-7)
- 1990-04-06: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE TESTING (91-6B-1)
- 1990-04-06: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE TESTING (90-6-107)
- 1990-04-06: SHIFTABILITY CONCERNS ON 5-SPEED MANUAL TRANSAXLE (90-7050-102)
- 1990-03-21: PARASITIC DRAIN ON BATTERY AMMETER CONNECTING PROCEDURE (90-6D-2)
- 1990-03-21: PARASITIC DRAIN ON BATTERY AMMETER CONNECTING PROCEDURE (90-8-170)
- 1990-03-15: MANUAL UPDATE-SEC. 6E1/6E2/6E3 CODE 33,34,63,64 (NON-TURBOS) (90-6E-15)
- 1990-03-15: MANUAL UPDATE-SEC. 6E1/6E2/6E3 CODE 33,34,63,64 (NON-TURBOS) (90-6-105)
- 1990-03-14: REPLACEMENT OF STRUT ASSY. 25MM STRUT ROD VS. 22MM ROD (88-3-27)
- 1990-03-14: SERVICE MANUAL UPDATE-SEC.6E2 REVISED TPS SPECIFICATIONS (89-6E-30)
- 1990-03-14: REPLACEMENT OF STRUT ASSY. 25MM STRUT ROD VS. 22MM ROD (90-3-117)
- 1990-03-14: SERVICE MANUAL UPDATE-SEC.6E2 REVISED TPS SPECIFICATIONS (90-622-101)
- 1990-03-13: FRT. SEAT BACK RATTLE @ PIVOT BOLT-NEW BOLT & BUSHING P/N'S (90-10-19)
- 1990-03-13: FRT. SEAT BACK RATTLE @ PIVOT BOLT-NEW BOLT & BUSHING P/N'S (90-2-159)
- 1990-03-09: INTERMITTENT TCC, NO TCC OR CODE 62/26 - SES LIGHT (90-7125-5)
- 1990-03-09: INTERMITTENT TCC, NO TCC OR CODE 62/26 - SES LIGHT (90-7125-108)
- 1990-02-16: INSTALL DAMPNER ON EXHAUST PIPE REAR OF THE CONVERTER (88-6F-5)
- 1990-02-16: INSTALL DAMPNER ON EXHAUST PIPE REAR OF THE CONVERTER (90-6-104)
- 1990-02-13: A/C R-12 SERVICE PROCEDURES CHARGING CAPACITY CHART (90-1-119)
- 1990-02-09: (SRTA) MODEL UPDATE W/3T40 (125C) (90-7125-6)
- 1990-02-06: SERVICE MANUAL UPDATE SEC. 6E-DRIVEABILITY & EMISS. (89-6E-28)
- 1990-02-06: SERVICE MANUAL UPDATE SEC. 6E-DRIVEABILITY & EMISS. (90-6-103)
- 1989-12-01: SERVICE MANUAL UPDATE PARKING BRAKE ADJUSTMENT (90-5-105)
- 1989-12-01: SERVICE MANUAL UPDATE PARKING BRAKE ADJUSTMENT (90-5-5)
- 1989-11-09: LOOSE CARPET ON SIDE WALL TRIM PADS (REPAIR PROCEDURE) (90-10-9)
- 1989-11-09: LOOSE CARPET ON SIDE WALL TRIM PADS (REPAIR PROCEDURE) (90-2-114)
- 1989-11-01: REVISED DRIVE LINK WEAR SPECIFICATION 125C - 440T4 (90-7-3A)
- 1989-11-01: REVISED DRIVE LINK WEAR SPECIFICATION 125C - 440T4 (90-7440-104)
- 1989-10-17: SLIPS IN 1ST AND/OR NO 1ST GEAR/NEW PISTON SEALS (89-7125-13)
- 1989-10-17: SLIPS IN 1ST AND/OR NO 1ST GEAR/NEW PISTON SEALS (89-7125-116)
- 1989-10-09: RADIO TELEPHONE/MOBILE RADIO INSTALLATION GUIDELINES (90-8-114)
- 1989-10-06: TIRE COMPANY WARRANTY ASSISTANCE PROGRAMS (90-3-3)
- 1989-09-27: SERVICE GUILD: USE OF FUEL WITH 15% MTBE IN ALL GM VEH. (89-0-7)
- 1989-08-18: HOOD WOBBLES WHEN OPEN DUE TO LOOSE HINGE PIVOT BOLTS (89-10-28)
- 1989-08-18: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE INFORMATION (90-6B-1)
- 1989-08-18: HOOD WOBBLES WHEN OPEN DUE TO LOOSE HINGE PIVOT BOLTS (89-2-195)
- 1989-08-18: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE INFORMATION (90-0-101)
- 1989-08-16: COLD ENGINE PISTON KNOCK ON 2.OL (NEW PISTON) (89-6-22)
- 1989-08-16: COLD ENGINE PISTON KNOCK ON 2.OL (NEW PISTON) (89-620-105)
- 1989-08-10: CFC REDUCTION AND REFRIGERANT RECOVERY (RECYCLING PROGRAM) (89-1-15)
- 1989-08-10: CFC REDUCTION AND REFRIGERANT RECOVERY (RECYCLING PROGRAM) (89-1-126)
- 1989-07-26: A/T TRANSAXLE FLUID COLOR LEVEL CHECK INFORMATION (89-7-6)
- 1989-07-26: A/T TRANSAXLE FLUID COLOR LEVEL CHECK INFORMATION (89-7-119)
- 1989-06-15: INCORRECT CRUISE CONTROL RESUME OPERATION (89-8-19)
- 1989-06-15: INCORRECT CRUISE CONTROL RESUME OPERATION (89-8-178)
- 1989-06-12: VIB. DIAG. USING A REED TACH. AND ROTATIONAL ORDER CHARTS (89-0-114)
- 1989-06-01: SPECIFICATIONS FOR HEAD BOLT TORQUE (88-6-123)
- 1989-05-29: SPECIAL POLICY: TEMPORARY REDUCTION/POWER STRG.-COLD (88-POL-4A)
- 1989-05-29: SPECIAL POLICY: TEMPORARY REDUCTION/POWER STRG.-COLD (9S02)
- 1989-05-25: SPECIAL POLICY: TEMPORARY REDUCTION OF POWER STRG.-COLD (88-POL-4)
- 1989-05-24: NEW PROCEDURE FOR REPLACEMENT OF FINAL DRIVE PINION (89-7-5)
- 1989-05-24: NEW PROCEDURE FOR REPLACEMENT OF FINAL DRIVE PINION (89-7-109)
- 1989-05-18: CHIPPED PAINT DIAGNOSIS AND REPAIR (89-10-22)
- 1989-05-18: CHIPPED PAINT DIAGNOSIS AND REPAIR (89-2-161)
- 1989-05-12: OIL FILTER LEAKAGE PROPER INSTALLATION PROCEDURE (90-6-5)
- 1989-05-12: OIL FILTER LEAKAGE PROPER INSTALLATION PROCEDURE (89-6-115)
- 1989-04-24: IMPROPER CRANKSHAFT SENSOR REPLACEMENT DUE TO OIL (89-631-105)
- 1989-04-19: POWER RACK & PINION GEAR SERVICE INFORMATION (89-3-17)
- 1989-04-19: SERVICE GUILD: CORRECT CABLE INSULATION FOR CABLE (WIRING) (89-8-14)
- 1989-04-19: SERVICE GUILD: CORRECT CABLE INSULATION FOR CABLE (WIRING) (89-8-162)
- 1989-04-18: DIAGNOSIS INFO ON THM 125C LO-REVERSE CLUTCH (89-7125-8)
- 1989-04-18: DIAGNOSIS INFO ON THM 125C LO-REVERSE CLUTCH (89-7125-109)
- 1989-04-14: GOODWRENCH VEHICLE SECURITY SYSTEM LABOR OPERATIONS (89-9-7)
- 1989-04-07: ACID RAIN PAINT LABOR OPERATIONS (89-LTG-1)
- 1989-04-03: BASE IDLE RPM ADJUSTMENT REVISED PROCEDURE AND SPEC. (88-6E-14)
- 1989-04-03: SERVICE GUILD: POWER STEERING FLUID (PROPER FLUID USAGE) (89-3-15)
- 1989-04-03: BASE IDLE RPM SETTING REVISED PROCEDURE & SPEC. (87-620-122)
- 1989-04-03: BASE IDLE RPM ADJUSTMENT REVISED PROCEDURE AND SPEC. (88-620-125)
- 1989-04-03: SERVICE GUILD: POWER STEERING FLUID (PROPER FLUID USAGE) (89-3-116)
- 1989-04-01: HIGH ACCELERATOR PEDAL EFFORT INOPERATIVE CRUISE CONTROL (88-9-10A)
- 1989-04-01: HIGH ACCELERATOR PEDAL EFFORT INOPERATIVE CRUISE CONTROL (88-628-141)
- 1989-03-27: COLD START ROUGHNESS/FAILURE TO RUN AFTER COLD START (87-620-121)
- 1989-03-21: INEFFECTIVE CRANKSHAFT SENSOR REPLACE-OIL ON SENSOR-W/(DIS) (89-6-10)
- 1989-03-21: INEFFECTIVE CRANKSHAFT SENSOR REPLACE-OIL ON SENSOR-W/(DIS) (89-628-111)
- 1989-02-27: FAILURE TO RUN COLD/HESITATES (NEW PROM MAY CORRECT) (88-620-124)
- 1989-02-21: RADIATOR LEAKS DUE TO WEAR FROM A/C LINE INSULATION (88-6B-4)
- 1989-02-21: RADIATOR LEAKS DUE TO WEAR FROM A/C LINE INSULATION (89-1-113)
- 1989-02-20: SPOOL VALVE SPLIT RINGS RACK AND PINION POWER STEERING (88-3-25)
- 1989-02-15: RATTLE/BUZZ FROM I/P DURING BRAKE APPLY AND RELEASE (90-5-8)
- 1989-02-15: RATTLE/BUZZ FROM I/P DURING BRAKE APPLY AND RELEASE (89-5-108)
- 1989-02-09: A/C REFRIGERANT LOSS DUE TO LOOSE/ MISSING ACCESS FIT. CAP (89-1-112)
- 1989-02-03: THM 400/475 PRODUCT UPDATE BOOK (89-7400-104)
- 1989-01-31: POOR AM OR FM RADIO RECEPTION ANT. COAX. FEMALE TERM. REPAIR (89-9-6)
- 1989-01-31: POOR AM OR FM RADIO RECEPTION ANT. COAX. FEMALE TERM. REPAIR (89-8-137)
- 1989-01-31: A/C HIGH SIDE SERVICE FITTING MISSING-REPLACE A/C HOSE ASSY. (8S09)
- 1989-01-30: FAILURE TO RUN COLD/HESITATES (NEW PROM MAY CORRECT) (89-6E-4)
- 1989-01-30: AXLE SEAL PROTECTOR TO PREVENT SEAL DAMAGE DURING INSTALL (89-7-2)
- 1989-01-30: SHIFT LEVER RATTLE/BUZZ NOISE IN 3RD. OR 4TH. GEARS ISUZU (89-7-3)
- 1989-01-30: FAILURE TO RUN COLD/HESITATES (NEW PROM MAY CORRECT) (89-620-103)
- 1989-01-30: AXLE SEAL PROTECTOR TO PREVENT SEAL DAMAGE DURING INSTALL (89-7-105)
- 1989-01-30: SHIFT LEVER RATTLE/BUZZ NOISE IN 3RD. OR 4TH. GEARS ISUZU (89-7050-100)
- 1989-01-24: USE HIGH CHARGER SETTING TO RECHARGE BATTERIES/PROCEDURE (89-6D-2)
- 1989-01-24: USE HIGH CHARGER SETTING TO RECHARGE BATTERIES/PROCEDURE (89-8-131)
- 1989-01-16: SERVICE MANUAL UPDATE TEMPERATURE SWITCH CONNECTOR (89-6D-1)
- 1989-01-16: SERVICE MANUAL UPDATE TEMPERATURE SWITCH CONNECTOR (89-8-115)
- 1989-01-10: SPECIAL POLICY: A/C HIGH SIDE SERVICE FITTING (88-POL-3)
- 1989-01-10: CAST ALUMINUM WHEEL POROSITY (REPAIR PROC. & SEALER) (89-3-105)
- 1988-12-26: SERVICE GUILD: FUEL PUMP STRAINER IN-TANK FILTER/SOCK (89-6C-8)
- 1988-12-26: SERVICE GUILD: FUEL PUMP STRAINER IN-TANK FILTER/SOCK (88-6-125)
- 1988-12-21: BRAKE PULSATION AND ON CAR BRAKE ROTOR TURNING (89-5-6)
- 1988-12-21: BRAKE PULSATION AND ON CAR BRAKE ROTOR TURNING (89-5-105)
- 1988-12-19: COLD START ROUGHNESS/FAILURE TO RUN AFTER COLD START (89-6E-26)
- 1988-12-19: COLD START ROUGHNESS/FAILURE TO RUN AFTER COLD START (88-620-123)
- 1988-11-03: NO SECOND GEAR THM 125C HYDRA-MATIC 3T40 (89-7125-3)
- 1988-11-03: NO SECOND GEAR THM 125C HYDRA-MATIC 3T40 (89-7125-102)
- 1988-11-02: FUEL FEED AND/OR RETURN PIPE REPAIR PROCEDURES (89-6C-2)
- 1988-11-02: FUEL FEED AND/OR RETURN PIPE REPAIR PROCEDURES (89-6-101)
- 1988-10-31: FREEZING DOOR LOCK CYLINDERS REPAIR PROCEDURE OUTLINED (88-2-234)
- 1988-10-19: V5 AIR CONDITIONING AND REFRIGERANT SYSTEM DIAGNOSTICS (89-1-5)
- 1988-10-19: V5 AIR CONDITIONING AND REFRIGERANT SYSTEM DIAGNOSTICS (89-1-110)
- 1988-10-10: BRAKE PULSATION REPLACE SLIDE PINS (88-5-17)
- 1988-10-10: SERVICE MANUAL UPDATE DRIVE AXLE REMOVAL PROCEDURE (89-3-5)
- 1988-10-10: BRAKE PULSATION REPLACE SLIDE PINS (88-5-137)
- 1988-10-10: SERVICE MANUAL UPDATE DRIVE AXLE REMOVAL PROCEDURE (89-4-101)
- 1988-10-07: NOISES CAUSED BY POWER STEERING CYLINDER LINE (89-3-4)
- 1988-10-07: BRAKE LEAD DIAGNOSIS INFORMATION (89-5-2)
- 1988-10-07: NOISES CAUSED BY POWER STEERING CYLINDER LINE (89-3-103)
- 1988-10-07: BRAKE LEAD DIAGNOSIS INFORMATION (89-5-101)
- 1988-09-24: REAR BRAKE ADJUSTMENT ACCESS HOLE(PROCEDURE TO REMOVE PLUG) (88-5-8A)
- 1988-09-24: REAR BRAKE ADJUSTMENT ACCESS HOLE(PROCEDURE TO REMOVE PLUG) (88-5-110)
- 1988-09-21: A/C HIGH PRESSURE SERVICE PORT (REMOVE CONTROL SWITCH) (88-1-13)
- 1988-09-21: A/C HIGH PRESSURE SERVICE PORT (REMOVE CONTROL SWITCH) (88-1-133)
- 1988-08-15: PROCEDURE FOR RELEASING PRODUCT SERVICE BULLETINS (88-0-111)
- 1988-08-15: TEMPERATURE SWITCH CONNECTOR SERVICE MANUAL UPDATE (88-8-173)
- 1988-08-08: ELECTROSTATIC DISCHARGE DAMAGE TO ECM (INFO. TO PREVENT) (88-8-168)
- 1988-08-08: FLUCTUATING TEMP GAGE FLASHING CHECK ENG. LIGHT (88-8-171)
- 1988-08-01: DELAYED OR INADEQUATE ENGINE COOLING AT IDLE WITH A/C ON (88-1-5A)
- 1988-08-01: DELAYED OR INADEQUATE ENGINE COOLING AT IDLE WITH A/C ON (88-620-106)
- 1988-07-25: REMOTE AIR CLEANER COVER LATCH BREAKAGE(REPAIR & P/N) (87-620-119)
- 1988-07-21: SERVICE MANUAL UPDATE TEMPERATURE SWITCH CONNECTOR (88-6D-5)
- 1988-07-21: SERVICE MANUAL UPDATE TEMPERATURE SWITCH CONNECTOR (88-620-122)
- 1988-07-18: SERVICE REPLACEMENT TRANSMISSION ASSEMBLY UPDATE (88-7-5)
- 1988-07-18: INTERMITTENT OR IN-OPERATIVE CENTER HIGH MOUNTED STOP LAMP (88-8-25)
- 1988-07-18: SERVICE REPLACEMENT TRANSMISSION ASSEMBLY UPDATE (88-7-108)
- 1988-07-18: INTERMITTENT OR IN-OPERATIVE CENTER HIGH MOUNTED STOP LAMP (88-8-170)
- 1988-07-06: SAGGING HEADLINER REPAIR PROCEDURE (88-10-38)
- 1988-07-06: SAGGING HEADLINER REPAIR PROCEDURE (88-2-208)
- 1988-06-28: REMOTE AIR CLEANER COVER LATCH BREAKAGE(REPAIR AND P/N) (87-6-28)
- 1988-06-28: REMOTE AIR CLEANER COVER LATCH BREAKAGE(REPAIR AND P/N) (88-620-121)
- 1988-06-23: 1-1 SHIFT DURING COLD WEATHER NEW ACCUMULATOR PISTON - P/N (88-7125-9)
- 1988-06-23: 1-1 SHIFT DURING COLD WEATHER NEW ACCUMULATOR PISTON - P/N (88-7125-109)
- 1988-06-14: SERVICE GUILD: SUSPENSION AND STEERING INFO. & DESCRIPTION (88-3-133)
- 1988-06-01: SPOOL VALVE SPLIT RINGS IN POWER STRG RACK & PINION GEARS (88-3-18)
- 1988-06-01: LOSS OF POWER ON 88 CAVALIERS (EXCEPT Z-24) LL8 OR LB6 (88-620-118)
- 1988-06-01: LOSS OF POWER ON 1988 CAVALIERS LL8 OR LB6 ENGINES (88-628-124)
- 1988-05-31: INTERMITTENT ECM CONNECTION MAY BE WEAK TERMINAL GRIP (88-6E-15)
- 1988-05-31: INTERMITTENT ECM CONNECTION MAY BE WEAK TERMINAL GRIP (88-6-116)
- 1988-05-26: SERVICE AND PARTS INFORMATION 125 FINAL DRIVE ASSEMBLY (88-7125-8)
- 1988-05-26: SERVICE AND PARTS INFORMATION 125 FINAL DRIVE ASSEMBLY (88-7125-108)
- 1988-05-19: CLEANING OF UPPER INSTRUMENT PANEL SURFACES (88-10-27)
- 1988-05-19: SERVICE GUILD: INSTALLATION OF AFTER MARKET STYLED WHEELS (88-3-16)
- 1988-05-19: CLEANING OF UPPER INSTRUMENT PANEL SURFACES (88-2-183)
- 1988-05-17: WATER LEAKS/ WET CARPET (MAY BE CLOGGED A/C DRAIN) (88-1-14)
- 1988-05-17: IDENTIFYING RACK AND PINION STEERING SYSTEM NOISES (88-3-19)
- 1988-05-17: WATER LEAKS/ WET CARPET (MAY BE CLOGGED A/C DRAIN) (88-1-135)
- 1988-05-17: IDENTIFYING RACK AND PINION STEERING SYSTEM NOISES (88-3-128)
- 1988-04-25: SPORADIC ENGAGEMENT OF THE TORQUE CONVERTER CLUTCH (88-7-3)
- 1988-04-25: SPORADIC ENGAGEMENT OF THE TORQUE CONVERTER CLUTCH (88-7-105)
- 1988-04-22: RATTLE OR BUZZ NOISE FROM THE INSTRUMENT PANEL (88-10-39)
- 1988-04-22: RATTLE OR BUZZ NOISE FROM THE INSTRUMENT PANEL (88-2-173)
- 1988-04-11: SERVICE MANUAL UPDATES PISTON TO BORE CLEARANCES (88-6-18)
- 1988-04-11: SERVICE MANUAL UPDATES PISTON TO BORE CLEARANCES (88-620-117)
- 1988-03-31: INSTALLATION PROCEDURE FOR RACK AND PINION STEERING GEARS (88-3-14)
- 1988-03-31: INSTALLATION PROCEDURE FOR RACK AND PINION STEERING GEARS (88-3-123)
- 1988-03-30: INTERMITTENT HIGH IDLE ON SHIFT TO DRIVE (88-6E-17)
- 1988-03-30: INTERMITTENT HIGH IDLE ON SHIFT TO DRIVE (88-620-114)
- 1988-03-21: GAS-TECH. INFO FROM THE CANADIAN GEN. STANDARDS BOARD (88-6-109)
- 1988-03-14: GARNISH MOLDING RATTLE INSTALL NEW RETAINER CLIPS (88-10-23)
- 1988-03-14: GARNISH MOLDING RATTLE INSTALL NEW RETAINER CLIPS (88-1-122)
- 1988-03-07: LOW COOLANT LIGHT, ERRATIC TEMP GAUGE (88-8-133)
- 1988-02-29: ENG. MISS,HESITATION & ROUGH PIERCED SEC. IGN. COMPONENTS (88-6-106)
- 1988-02-26: DELAYED NEUTRAL TO DRIVE ENGAGEMENT (88-7125-7)
- 1988-02-26: DELAYED NEUTRAL TO DRIVE ENGAGEMENT (88-7125-105)
- 1988-02-23: HEAT SHIELD IMPORTANCE REINSTALLATION REPAIR (88-6F-1)
- 1988-02-23: HEAT SHIELD IMPORTANCE REINSTALLATION REPAIR (88-6-108)
- 1988-02-22: COLD WEATHER STARTING PROCEDURE DESCRIBED (88-6-11)
- 1988-02-22: COLD WEATHER STARTING PROCEDURE DESCRIBED (88-620-113)
- 1988-02-19: NIBRON COATED INPUT CARRIER THRUST WASHERS W/125-125C (88-7125-6)
- 1988-02-19: NIBRON COATED INPUT CARRIER THRUST WASHERS W/125-125C (88-7125-104)
- 1988-02-15: MANUAL TRANSMISSION REPAIR PROCEDURES (88-7050-105)
- 1988-02-10: LEAD OR PULL ON STRAIGHT AFTER MAKING TURN (88-3-10)
- 1988-02-10: LEAD OR PULL ON STRAIGHT AFTER MAKING TURN (88-3-115)
- 1988-02-04: ODOR FROM A/C AT START-UP PROCEDURE TO REPAIR DESCRIBED (90-1-1)
- 1988-02-01: SERVICE GUILD: A/C COMPRESSOR BOLT/STUD TORQUE LOSS (REPAIR (88-1-6A)
- 1988-02-01: SERVICE GUILD: A/C COMPRESSOR BOLT/STUD TORQUE LOSS (REPAIR (88-1-114)
- 1988-01-26: SCAN TOOL WORKSHEET AID TO DIAGNOSIS (88-6-105)
- 1988-01-25: CORRECT OIL PRESSURE READING DIAGNOSIS AND SWITCH P/N (88-8-119)
- 1988-01-15: TAILGATE POWER LOCK WILL NOT FULLY OPEN DOOR- WAGON (88-10-36)
- 1988-01-15: TAILGATE POWER LOCK WILL NOT FULLY OPEN DOOR- WAGON (88-2-131)
- 1988-01-14: DIFFICULTY OPENING HOOD NEW SPRING FOR HIGHER LIFT (88-2-1)
- 1988-01-14: DIFFICULTY OPENING HOOD NEW SPRING FOR HIGHER LIFT (88-2-130)
- 1988-01-11: PART WARRANTY CLAIM SUBMISSION REVISED FOR NON DIV. VEHICLES (88-POL-2)
- 1988-01-11: REMOVAL OF CHEMICAL SPOTTING AND MINOR PAINT IMPERFECTIONS (88-10-11)
- 1988-01-05: REVISED SPARK PLUG RECOMMENDATIONS (87-6E-26)
- 1988-01-05: REVISED SPARK PLUG RECOMMENDATIONS (88-620-110)
- 1988-01-04: ASSEMBLY PLANT PAINT SUPPLIER INFORMATION (88-10-6)
- 1988-01-04: ENGINE STALLS WHILE ENGAGING IN REVERSE OR DRIVE (88-7125-2)
- 1988-01-04: ASSEMBLY PLANT PAINT SUPPLIER INFORMATION (88-2-124)
- 1988-01-04: ENGINE STALLS WHILE ENGAGING IN REVERSE OR DRIVE (88-7125-102)
- 1987-12-15: TRANSMISSION VALVE BODY COVER/OIL PAN LEAKS (88-7125-1)
- 1987-12-15: TRANSMISSION VALVE BODY COVER/OIL PAN LEAKS (88-7125-100)
- 1987-12-10: REVISED LABOR OPERATIONS FOR DRIVEABILITY DIAGNOSIS (88-6E-4)
- 1987-12-08: FRONT POWER DOOR LOCKS STICKS OR BINDS (88-10-10)
- 1987-12-08: FRONT POWER DOOR LOCKS STICKS OR BINDS (88-2-125)
- 1987-12-03: AC DELCO RADIO REPAIR NEW CAR LIMITED WARRANTY (88-9-1)
- 1987-12-01: DAMAGE TO WIRING TERMINALS ON ENGINE SENSORS-METRI-PACK 150 (88-8-6)
- 1987-12-01: DAMAGE TO WIRING TERMINALS ON ENGINE SENSORS-METRI-PACK 150 (88-8-117)
- 1987-11-24: SPECIALIZED A/C ORIFICE TUBE AND LOCATION (88-1-4)
- 1987-11-24: SPECIALIZED A/C ORIFICE TUBE AND LOCATION (88-1-105)
- 1987-11-16: DELCO BATTERY STORAGE TESTING DIAGNOSIS AND CHARGING (87-8-5)
- 1987-11-16: TIRE WARRANTIES IRREGULAR/PREMATURE WEAR (88-3-5)
- 1987-11-16: TIRE WARRANTIES IRREGULAR/PREMATURE WEAR (88-3-104)
- 1987-11-16: DELCO BATTERY STORAGE TESTING DIAGNOSIS AND CHARGING (89-8-109)
- 1987-10-29: DELAYED A/C COOLING AFTER START UP (88-1-1)
- 1987-10-29: SERVICE BRAKE PART NUMBER (REDUCES PEDAL EFFORT) (88-5-2)
- 1987-10-29: DELAYED AIR CONDITION COOLING AFTER START UP (88-1-102)
- 1987-10-29: DELAYED A/C COOLING AFTER START UP (88-1-108)
- 1987-10-29: SERVICE BRAKE PART NUMBER (REDUCES PEDAL EFFORT) (88-5-106)
- 1987-10-20: SERVICE GUILD: ENGINE MISS/ BACKFIRE/HES. POOR ENG. GROUND (87-6-22)
- 1987-10-20: BRAKE SYSTEM CHANGE/ IMPROVED ASSIST (88-5-4)
- 1987-10-20: SERVICE GUILD: ENGINE MISS/ BACKFIRE/HES. POOR ENG. GROUND (88-620-105)
- 1987-10-19: INSTRUMENT CLUSTER EXCHANGE PROGRAM INFORMATION (88-8-106)
- 1987-10-12: BUICK NEW VEHICLE ANNOUNCEMENT MANUAL AND LABEL ORDERING (88-0-1A)
- 1987-09-24: ECM AND BCM MODULE EXCHANGE PROGRAM (87-6E-2)
- 1987-09-24: ECM AND BCM MODULE EXCHANGE PROGRAM (87-8-100)
- 1987-09-24: INSTRUMENT CLUSTER EXCHANGE REPAIR PROGRAM (89-8-112)
- 1987-09-22: ACRYLIC COATING TOUCH UP PAINT NEW PRODUCT ORDER INFORMATION (88-10-2)
- 1987-09-08: RETIGHTEN FUEL METER BODY ATTACHING SCREWS ON TBI 700 (89-6C-4)
- 1987-09-08: RETIGHTEN FUEL METER BODY ATTACHING SCREWS ON TBI 700 (89-620-101)
- 1987-09-07: FRENCH LABEL INSTALLATION INSTRUCTIONS (PASS. CARS) (88-0-100)
- 1987-09-01: RETIGHTEN FUEL METER BODY ATTACHING SCREWS ON TBI 700 (87-6-118)
- 1987-09-01: INSTRUMENT CLUSTER EXCHANGE REPAIR PROGRAM (88-8-107)
- 1987-08-20: STEERING LEAD OR PULL DIAGNOSIS AND POSSIBLE REPAIR (87-3-132)
- 1987-08-18: ROUGH IDLE, STALL, COLD START ENG. NOISE, HESITATE, NO POWER (88-620-100)
- 1987-07-31: WARRANTY CLAIMS PROCESSING INFORMATION (88-POL-1)
- 1987-07-22: CHECKING PROPER FLUID LEVEL PROCEDURE (88-7-1)
- 1987-07-22: CHECKING PROPER FLUID LEVEL PROCEDURE (88-7-100)
- 1987-06-03: TIRE COMPANY ASSISTANCE PROGRAM (87-3-11)
- 1987-05-14: DIAGNOSIS OF NOISE FROM REAR MAIN SEAL (87-6-15)
- 1987-05-14: DIAGNOSIS OF NOISE FROM REAR MAIN SEAL (87-6-114)
- 1987-04-07: METHOD OF VERIFYING ' GOOD ELECTRICAL SYSTEM GROUND ' (87-8-139)
- 1987-03-16: CAST ALUMINUM WHEEL POROSITY REPAIR AND SEALER REVISED (89-3-7)
- 1987-03-16: CAST ALUMINUM WHEEL POROSITY REPAIR AND SEALER REVISED (87-3-115)
- 1986-12-15: INSTRUMENT CLUSTER EXCHANGE PROGRAM INFORMATION (87-8-113)
- 1986-10-20: USE OF UNLEADED GASOLINE IN VEHICLES USING LEADED GAS (87-6-100)
- 1986-09-23: USE OF UNLEADED GASOLINE VEHICLES USING LEADED GAS (87-0-104)
- 1986-09-22: DELCO FREEDOM BATTERY STORAGE AND TESTING (87-8-3)
- 1986-09-22: DELCO FREEDOM BATTERY STORAGE AND TESTING (87-8-108)
- 1986-08-28: SERVICE GUILD: ELECTROSTATIC DISCHARGE DAMAGE (86-8-15)
- 1986-08-28: SERVICE GUILD: ELECTROSTATIC DISCHARGE DAMAGE (87-8-102)
- 1985-10-23: DA6 A/C COMPRESSOR REPAIR REPAIR ASSEMBLY P/N (86-1-1)
- 1985-10-23: DA6 A/C COMPRESSOR REPAIR REPAIR ASSEMBLY P/N (86-1-100)
- 1985-10-07: CRACKED PAINT USING RM HIGH SOLIDS RAPID FILTER (86-2-103)