COWL WATER LEAKS SEALING COWL SEAMS. Buick Skyhawk 1983

For 1990-2009 cars

# COWL WATER LEAKS SEALING COWL SEAMS

#### MODELS AFFECTED: 1983 Skyhawk

Water entering the passenger compartment from the cowl area of a 1983 Skyhawk may be corrected by sealing the cowl seams shown in illustrations, as necessary.

The air conditioning evaporator drain must be checked carefully to make sure it is open and does not restrict water flow.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.