ROAR NOISE IN CLUTCH CABLE TO CLUTCH BRACKET. Buick Skyhawk 1983

For 1990-2009 cars

# ROAR NOISE IN CLUTCH CABLE TO CLUTCH BRACKET

#### VEHICLES AFFECTED: 1983 'J' SERIES VEHICLES EQUIPPED WITH MANUAL TRANSMISSION WHEN DIAGNOSING A CONDITION OF A 'ROARING' TYPE NOISE IN EARLY BUILT 1983 'J' SERIES VEHICLES EQUIPPED WITH A MANUAL TRANSMISSION, BE SURE TO EXAMINE THE CLUTCH CABLE FOR PROPER ATTCHMENT TO THE CLUTCH BRACKET AS SHON IN FIG. 1. THE CLUTCH CABLE SHOULD BE PUSHED DOWN AS FAR AS POSSIBLE INTO THE RUBBER ISOLATOR LOCATED ON TOP OF THE CLUTCH BRACKET. IF THE CABLE IS NOT PROPERLY POSITIONED IN THE RUBBER ISOLATOR AN OBJECTIONABLE CLUTCH 'ROARING' NOISE MAY BE PRODUCED.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.