SERVICE MANUAL UPDATE TEMPERATURE SWITCH CONNECTOR. Buick Skyhawk 1988

For 1990-2009 cars

# SERVICE MANUAL UPDATE TEMPERATURE SWITCH CONNECTOR

SERVICE MANUAL UPDATE - 2.0L (VIN 1) ENGINE METAL TEMPERATURE SWITCH CONNECTOR

#### MODELS AFFECTED: 1988 SKYHAWKS WITH 2.0L OHV ENGINES (VIN 1) ---------------- The engine metal temperature switch that was used on Skyhawks with the 2.0L (VIN 1) engine, was eliminated in 1988. An illustration in Section 625((Engine Wiring) incorrectly points to a "metal temperature switch connector item 9) on Buick 1988 2.0L (VIN 1) engine supplement, Page 6D5-1, Figure 1.

Please draw a line through the legend and the art at Item 9 on your copy of the service manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.