FRONT LICENSE PLATE- BRACKET INSTALL. Buick Skyhawk 1982

For 1990-2009 cars

# FRONT LICENSE PLATE- BRACKET INSTALL

#### MODELS AFFECTED: 1982 Skyhawk

Due to mislocated dimples in the Skyhawk front bumper fascia, it will be necessary to mark new hole locations as follows:

1. Draw a line between the two lower dimples using a flexible ruler or straight edge as a guide. Illustration.

2. Draw a line between the two upper dimples.

3. Measure inboard 20mm (13/16") from each of the four dimples and mark a new hole location on the line.

4. Drill four (4) llmm (7/16") diameter holes at these newly marked locations and install the moly-nuts.

Complete the license plate bracket installation, following the instructions in the package.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.