SERV MAN UPDT-SEC.6A1,6C,6E2 FUEL PRESSURE RELIEF. Buick Skyhawk 1988

For 1990-2009 cars

# SERV MAN UPDT-SEC.6A1,6C,6E2 FUEL PRESSURE RELIEF

#### SUBJECT: SERVICE MANUAL UPDATE/SECTIONS 6A1, 6C, 6E2 - REVISED FUEL PRESSURE RELIEF PROCEDURE

#### MODELS AFFECTED: 1988 SKYHAWK MODELS WITH 2.OL ENGINE (VIN CODE K)

This bulletin applies to the 1988 Skyhawk Service Manual. Sections 6Al (2.OL OHC ENGINE), 6C (ENGINE FUEL), and 6E2 (DRIVEABILITY AND EMISSIONS-TBI) contain incorrect fuel system pressure relief procedures.

The Throttle Body Injection (TBI) unit used on this engine contains a constant bleed in the fuel meter assembly which allows fuel pressure to bleed down when the engine is turned "OFF". Following is the correct fuel pressure relief procedure for this system:

#### FUEL PRESSURE RELIEF PROCEDURE:

#### CAUTION:

- To reduce the risk of fire and personal injury, relieve the fuel system pressure before servicing fuel system components.

- After relieving system pressure, a small amount of fuel may be released when servicing lines or connections. To reduce the chance of personal injury, cover fuel line fittings with a shop towel before disconnecting to catch any fuel that may leak out. Place the towel in an approved container when disconnect is completed.

1. Disconnect negative battery terminal to avoid possible fuel discharge if an accidental attempt is made to start the engine.

2. Loosen fuel filler cap to relieve tank vapor pressure.

3. The internal constant bleed feature of TBI Model 700 relieves fuel pump system pressure when the engine is turned "OFF". Therefore, no further steps are required.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.