THROTTLE BODY INSTALLATION REVISED TORQUE SPEC.. Buick Skyhawk 1984

For 1990-2009 cars

# THROTTLE BODY INSTALLATION REVISED TORQUE SPEC.

THE INSTALLATION TORQUE OF TWO THROTTLE BODY ATTACHING BOLTS AND NUT ON STUD HAS BEEN CHANGED TO 23 N.M (17 FT. LBS.). PLEASE NOTE THIS CHANGE IN YOUR COPY OF THE "J" SERIES SHOP MANUAL (ST-366-84, ST-366-85 AND ST-388-85) PAGE 6C15-5 TBI INSTALLATION STEP 6.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.