FRONT POWER DOOR LOCKS STICKS OR BINDS. Buick Skyhawk 1988

For 1990-2009 cars

# FRONT POWER DOOR LOCKS STICKS OR BINDS

#### MODELS AFFECTED: 1982-88 SKYHAWKS WITH POWER DOOR LOCKS

Skyhawks with power door locks may have a condition of sticking or binding of the front door lock(s) when operating the power lock option.

The condition may be repaired by removing the trim pad and crimping the bellcrank butterfly opening as shown in the illustration.

Crimp the opening about 2m (5/64") at a time and try the lock operation after each crimp until satisfactory operation is achieved.

#### WARRANTY INFORMATION

Labor Operation Number: C3348 RH C3358 LH Labor Time: Use Applicable Time Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.