POOR A/C PERFORMANCE OR LEAK (MAYBE LEAK FROM HOSE). Buick Skyhawk 1986

For 1990-2009 cars

# POOR A/C PERFORMANCE OR LEAK (MAYBE LEAK FROM HOSE)

LOSS OF A/C PERFORMANCE DUE TO WORN A/C HOSE ASSEMBLY

#### VEHICLES AFFECTED: 1986 BUICK AND PONTIAC MODELS WITH LA5 ENGINE ----------------- (1.8 OHC TURBO) WITH C60

Some 1986 Buick and Pontiac models equipped with the LA5 Engine (1.8 OHC Turbo) and C60 may experience a leaking A/C suction/discharge hose assembly due to the hoses coming in contact with each other.Check hose assembly for abrasion or rub through, and replace if necessary with part number 10040317.

#### NOTICE: Hose assembly should have a 25 mm (1 inch) clearance between the hoses and if necessary, bend the pipes to assure this clearance. Refer to illustration.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.