INOPERATIVE LOW COOL LIGHT LIGHT OPERATION OUTLINED. Buick Skyhawk 1987

For 1990-2009 cars

# INOPERATIVE LOW COOL LIGHT LIGHT OPERATION OUTLINED

#### VEHICLES AFFECTED: 1987 2.0L L-4 (VIN CODE 1) J CAR

During the 1987 model year, a change has been made to the low engine coolant light system of the 2.0L L-4 (VIN Code 1)"J" cars. The light will no longer illuminate on the instrument panel at low coolant levels on the following vehicles after the VIN breakpoints stated:

Dealers should not attempt to repair or alter this as-built condition.

Division VIN Breakpoint (Last 7 Digits)

Chevrolet 7164718 Chevrolet J182691 Chevrolet K136117 Buick K436904 Oldsmobile K318696

This bulletin is for informational purposes only.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.