SERVICE MANUAL UPDATE TEMPERATURE SWITCH CONNECTOR. Buick Skyhawk 1988

For 1990-2009 cars

# SERVICE MANUAL UPDATE TEMPERATURE SWITCH CONNECTOR

#### MODELS AFFECTED: 1988-1989 SKYHAWKS WITH 2.0L ENGINES (VIN CODE 1)

The engine metal temperature switch that was used on the Skyhawk/Skylark carline, with the 2.0L (VIN Code 1) engine, was eliminated in 1988. An illustration in Section 6D5 (engine wiring) incorrectly points to a "metal temperature switch connector" (item 9) in the following service manuals: 1988 Buick 2.0L (Vin Code 1) Engine Supplement, Page 6D5-1, Figure 1.

1989 Buick Skyhawk and Skylark New Product Service Manual, Page 6D5-1, Figure 1.

Please draw a line through the legend and the art at item 9 on your copy of the service manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.