REVISED FRONT WHEEL TOE SPECIFICATION MANUAL REVISION. Buick Skyhawk 1985

For 1990-2009 cars

# REVISED FRONT WHEEL TOE SPECIFICATION MANUAL REVISION

VEHILES AFFECTED: 1985 'J' and 'N' Models

The front wheel toe Service Setting has been revised to -.06 degrees per wheel on 1985 'J' and 'N' models. Please make this correction in section 3A of the 1985 Service Manuals.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.