TORQUE ROD REMOVAL BODY MANUAL REVISION. Buick Skyhawk 1983

For 1990-2009 cars

# TORQUE ROD REMOVAL BODY MANUAL REVISION

#### MODELS AFFECTED: 1983 Skyhawk

The 1983 Fisher Body Service Manual for Skyhawks omitted the torque rod removal and installation procedure. This procedure should be incorporated in Section 7, Page 7-2 of the 1983 Body Service Manual.

SKYHAWK TORQUE ROD REMOVAL AND INSTALLATION

1. Raise rear compartment lid and prop open.

2. Remove right and left quarter wheelhouse trim on style so equipped.

3. Using tool J-21412 or equivalent, disengage torque rod end from bracket and allow rod to slowly unwind. Disengage opposite end of rod from hinge and remove rod. Repeat on other side (Figure 7-2).

4. To install, reverse removal procedure, check for proper lid operation, and adjust torque rods as required. Replace any trim removed.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.