POWER STEERING FLUID LEAKAGE FROM RESERVOIR. Buick Somerset 1985

For 1990-2009 cars

# POWER STEERING FLUID LEAKAGE FROM RESERVOIR

#### VEHICLES AFFECTED: 1985 'N' Series Vehicles

Some 1985 'N' series vehicles built prior to November of 1984 may exhibit power steering fluid seepage from the reservoir fill cap area. This condition may be repaired by replacing the capstick with a new capstick and baffle. Place the baffle inside the filler neck and install new capstick as shown in Fig. 1.

New capstick and baffle package part numbers are:

V-6 Engine (VIN Code L) - 7849388

4-Cyl. Engine (VIN Code U) - 7849387

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.