REVISED FRONT WHEEL TOE SPECIFICATION MANUAL REVISION. Buick Somerset 1985

For 1990-2009 cars

# REVISED FRONT WHEEL TOE SPECIFICATION MANUAL REVISION

#### Models Affected: 1985 Skyhawk and Somerset Regal

The front wheel toe Service Setting has been revised to -.06 degrees per wheel on 1985 Skyhawk and Somerset Regal models. Please make this correction on page 3A-9 of the 1985 Buick Chassis Service Manual, Volume 1.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.