HEADLAMP BEZEL REMOVAL PROCEDURE. Buick Somerset 1986

For 1990-2009 cars

# HEADLAMP BEZEL REMOVAL PROCEDURE

#### VEHICLES AFFECTED: 1986 Oldsmobile Calais

It has come to our attention that 1986 Calais headlamp bezels are being damaged during removal for lamp replacement. The following procedure should be used to remove the bezel:

1. Remove two (2) retaining screws at top of bezel.

2. Gently tip the top of the bezel forward enough to allow insertion of a flat bladed screwdriver. See Figure 1.

3. Position blade of screwdriver as shown in view A of Figure 1 and twist.

Should the clip shown in View A require replacement, order part number 22528265.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.