TRANSMISSION CONVERTER COVER CORRECT PLACEMENT. Buick Somerset 1985

For 1990-2009 cars

# TRANSMISSION CONVERTER COVER CORRECT PLACEMENT

WHEN REPLACING THE TRANSMISSION CONVERTER (FLEXPLATE) COVER ON THE ABOVE VEHICLES CARE SHOULD BE TAKEN TO INSTALL THE TABS ON THE COVER ON THE ENGINE SIDE OF THE ENGINE OIL PAN FLANGE TO PREVENT POSSIBLE INTERFERENCE WITH THE FLEXPLATE. SEE ILLUSTRATION. AS FURTHER AID IN PREVENTING INTERFERENCE IN THIS AREA A SNAP IN PIN LOCK RETAINER PART NUMBER 5973400 IS BEING INSTALLED IN THE COVER IN PRODUCTION. ITS SUGGESTED THAT THIS PIN BE INSTALLED IN THE EXISTING OPENING OF ANY COVER, NOT SO EQUIPPED, PRIOR TO REINSTALLING IT. SEE ILLISTRATION.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.