FRONT STABILIZER BAR INSULATOR BUSHING SQUEAK. Buick Somerset 1985

For 1990-2009 cars

# FRONT STABILIZER BAR INSULATOR BUSHING SQUEAK

STABILIZER BAR INSULATOR BUSHING SQUAWK

#### MODELS AFFECTED: 1985-86 SKYHAWK & SOMERSET --------------- 1986 SKYLARK

A squawk noise from the front stabilizer bar insulator bushings may be corrected by installing new Teflon lined bushings. The new bushings are being used in production beginning approximately February 1, 1986.

Bushing part numbers and applications are shown below:

#### Stabilizer Bar Bushing 24mm Shaft Diameter

Part Number 22532210 (Replaces No. 14085145). 1985-86 Skyhawk with standard suspension. 1985-86 Somerset & 1986 Skylark with 2.5L engine.

#### Stabilizer Bar Bushing 28mm Shaft Diameter

Part Number 22532212 (Replaces No. 14085147). 1985-86 Skyhawk with F40 or F41 suspension. 1985-86 Somerset & 1986 Skylark with 2.5L engine and F41 or with 3.0L engine.

#### Stabilizer Bar Bushing 30mm Shaft Diameter

Part Number 22532213 (Replaces No. 14085148). 1985-86 Skyhawk with FE2. 1985-86 Somerset and 1986 Skylark with 3.0L engine and F41.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.