NEW REVERSE AND 1-2 BAND APPLY PIN GAGE. Cadillac Allante 1990

For 1990-2009 cars

# NEW REVERSE AND 1-2 BAND APPLY PIN GAGE

#### MODELS AFFECTED: 1989-1990 DE VILLES, FLEETWOODS, ELDORADOS, SEVILLES, AND ALLANTES

A new reverse band apply pin gage, J-33382-10, will be available approximately October 15, 1989 to service all 1989 and 1990 THM 440-T4/4T60 transaxles. In addition, the gage can be used to select the reverse band pin and the 1-2 band apply (servo) pin on all 1989 and 1990 THM F-7 transaxles. J-33382-10 has a hex head for easy identification.

#### IMPORTANT: DO NOT USE PIN GAGE J-33382-10 ON 1988 OR PRIOR MODELS. CONTINUE TO USE J-33382-2 ON 1988 OR EARLIER MODELS.

#### IMPORTANT: Pin gage J-33382-2 may be used on 1989-1990 models until the new gage (J-33384-10 is available. When using J-33382-2 on 1989-1990 models, select the apply pin which is two sizes longer than indicated by the gage.

#### Service Manual Reference:

This product change information will be shown in the Automatic Transaxle Unit Repair Section of the 1990 Service Information Manual.

#### Service Tool Information:

The reverse band apply pin gage, J-33382-10, will be available approximately October 15, 1989 from Kent-Moore. It can be ordered through their order department at (313) 574-2332 or 1-800-345-2233.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.