BACK LIGHT REAR DEFOGGER CONNECTOR DIFFICULT. Cadillac Allante 1987

For 1990-2009 cars

# BACK LIGHT REAR DEFOGGER CONNECTOR DIFFICULT

BACKLIGHT REAR DEFOGGER CONNECTOR DIFFICULT TO DISCONNECT FROM HARDTOP

#### VEHICLES AFFECTED: 1987 ALLANTE -----------------

Some 1987 Allante backlight rear defogger connectors may be difficult to disconnect from the hardtop. To repair this condition, use the following procedure:

1. Disconnect the backlight rear defogger connector (male connector) from the hardtop or soft top (see Figure 1).

2. Remove and discard the green connector seal (see Figure 2).

3. Remove the locking tab with a sharp tool, cutting it flush to the connector surface (see Figure 2).

4. Reconnect backlight rear defogger.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.