SERVICE MANUAL UPDATE-SEC. 5 BRAKE ROTOR SPECIFICATIONS. Cadillac Allante 1992

For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 5 BRAKE ROTOR SPECIFICATIONS

#### SUBJECT: SECTION 6 BRAKE ROTOR SPECIFICATIONS

VEHICLES AFFECTED: 1992-93 "E/K/V" MODELS

This bulletin is an update to Section 5, Brake Rotor Specification, for the E, K, and V series. The corrections listed below are for 1992-1993 Service Information Manuals. Please mark these corrections in your manuals.

1992-1993 All E, K, and V

#### Front Rotor:

0 Rotor thickness (new) should be 32.20mm (1.268"). 0 Minimum rotor thickness after refinish should be 31.08mm (1.224").

#### Rear Rotor:

0 Minimum rotor thickness after refinish should be 9.88mm (.389").

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.