CLUNK/RATTLE AT LEFT FRT. CNR. (DIAG./REPL./SECURE RTRN. LINE. Cadillac Allante 1992

For 1990-2009 cars

# CLUNK/RATTLE AT LEFT FRT. CNR. (DIAG./REPL./SECURE RTRN. LINE

#### SUBJECT: CLUNK OR RATTLE AT LEFT FRONT CORNER OF CAR (DIAGNOSE/REPLACE OR SECURE RETURN LINE)

#### VEHICLES AFFECTED: 1992 "E, K, V" MODELS

Some 1992 Cadillac Eldorados, Sevilles, and Allantes may experience a clunk or rattle condition at the left front corner of the car due to the power steering left-hand return line contacting the transaxle case.

To repair this condition inspect the left-hand return line. If the return line shows wear as a result of the contact, it should be replaced per Service Information Manual procedures in Section 3B. If no wear is evident, secure the left-hand return line to the cradle just forward of the left transaxle mount with a plastic tie strap as shown in Figure 1. If the left-hand return line is replaced, the new line should be secured to the frame with a plastic tie strap.

For vehicles repaired under warranty use:

Labour Operation: Labour Time: ---------------- ----------- Securing the line to the cradle only 0.3 hour

Left-hand return line - replace E8625 0.8 hour (Eldorados and Sevilles) 0.6 hour (Allantes)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.