CONVERTIBLE TOP BOOT WELL SEAL REPAIR LOOSE SEAL W/ADHESIVE. Cadillac Allante 1991

For 1990-2009 cars

# CONVERTIBLE TOP BOOT WELL SEAL REPAIR LOOSE SEAL W/ADHESIVE

#### SUBJECT: BOOT WELL OPENING SEAL FALLS OFF (SECURE SEAL TO FLANGE WITH WEATHERSTRIP ADHESIVE)

#### VEHICLES AFFECTED: 1987-1991 'V' MODEL

Some 1987-1991 Allantes may experience a condition of the boot well opening seal falling off or being pulled loose by operating the boot cover. To repair this condition secure the seal to the flange with 3M 08011 weatherstrip adhesive or equivalent. Refer to Figure 1.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.