SOFT TOP REAR GLASS-NEW PART SERVICE INFO & NEW PART NUMBER. Cadillac Allante 1989

For 1990-2009 cars

# SOFT TOP REAR GLASS-NEW PART SERVICE INFO & NEW PART NUMBER

#### SUBJECT: ALLANTE SOFT TOP REAR GLASS SERVICE PART

After February 1, 1991, only one part number will be serviced for all model years of Allante soft top rear glass. P/N 3635375 will be supplied with the following instructions for installation:

#### For 1987 Model Year:

1. Remove rear pull-down hook on new glass frame and install existing hook from part being removed from car.

2. Remove upper hinge rubber bumpers and adjustment screws and discard.

#### For 1988 Through Early 1990 (Phase I)

1. Remove upper hinge rubber bumpers and adjustment screws and discard.

#### For Late 1990 through 1991 (Phase II)

1. Install back glass as received.

#### NOTE: Phase I tops have manual latches on the front bow. Phase 11 tops have electric pull downs to latch the front bow.

Parts are currently available from GMSPO.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.