DOOR WINDOW BIND OR SLOW (SERVICE PROCEDURE). Cadillac Allante 1988

For 1990-2009 cars

# DOOR WINDOW BIND OR SLOW (SERVICE PROCEDURE)

#### SUBJECT: SERVICE PROCEDURE - DOOR WINDOWS BINDING OR SLOW

#### VEHICLES AFFECTED: 1987-92 "V" MODELS

THIS BULLETIN SUPERSEDES AND REPLACES CORPORATE BULLETIN REFERENCE NUMBER 811523.** THIS BULLETIN IS BEING REVISED TO INCLUDE 1989-1992 MODEL YEARS.

Some 1987-1992 Cadillac Allantes may experience a condition of slow operating or binding door windows. This condition may be more noticeable in colder outside temperatures. To repair this condition, use the following service procedure:

1. Remove lower door trim panel. (Refer to Section 10-5 of the Allante Service Information Manual).

2. Mark window location to sash around the three attaching bolts.

3. Postion the lower regulator attaching flange so the attaching bolts are approximately centred in the slotted holes, refer to Figure 1 Item 6.

#### NOTE: After performing each step run window and verify if condition is still present; if not, proceed to next step.

4. Loosen the two 10mm bolts on the bottom of the guide block and apply pressure outward on the sash, moving it as far outboard as possible, and tighten the bolts. (Refer to Figure 1, Item 8.)

5. Inspect the upstop adjustment. Adjust the upstop so threads show at the top and bottom where it is threaded through the regulator block, refer to Figure 1 item 2. If the upstop requires adjustment, the glass must be adjusted up or down as needed to ensure good sealing to the roof weatherstrip. Adjust the glass by loosening the three attaching bolts, moving the glass and tightening the bofts. Mark the new location of the glass on the sash.

6. Remove the door glass and inspect the aluminum guide that is bonded to the front of the glass. Sight down the length of the glass from top to bottom and verify that the contour of the guide matches the contour of the glass, refer to Figure 2. Cover the guide with masking tape to protect the guide appearance; and reform the guide with hammer and dolly or pliers to match the contour of the glass, refer to Figure 3.

7. Inspect the leading edge of the guide for wear. The guide is designed for inboard and outboard support of the glass only and should not contact the leading edge of the run channel felt strip. To eliminate the possibility of the guide "bottoming out" in the run channel, file or grind 4mm off the entire front edge of the guide. Use a strip of masking tape as a guide, refer to Figure 4. Smooth all sharp edges and mund off corners to prevent the guide from "digging in" to the run channel felt strip.

8. Remove the run channel felt strip and inspect for wear, cuts, bunching up, or separating at the center seam. If any of problems are noted, replace the run channel felt strip.

9. Reinstall the door window relocating it in itss last marked position to the sash. If no improvement in condition is noted, replace the regulator and verify all previous adjustments.

#### WARRANTY INFORMATION:

For vehicles repaired under warranty use:

Labour Time: 1.2 hours (Left) 1.2 hours (Right)

** BULLETIN REFERENCES: Corporate Ref. 811523

General Motors of Canada 88-2-227

Cadillac Division T-89-12

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.