REVISION-TRANSAXLE MOUNT FASTENER TORQUE VALVES THM F-7. Cadillac Allante 1987

For 1990-2009 cars

# REVISION-TRANSAXLE MOUNT FASTENER TORQUE VALVES THM F-7

#### MODELS AFFECTED: 1987-1988 ALLANTES

Two right side transaxle mount fastener torque values indicated in Figure 7Al-37 on page 7Al-31 of the 1987-1988 Allante Service Information Manual are incorrect. Fasteners torqued to the indicated values could result in damage to the transaxle mount. Correct torque values are listed below:

Item Indicated Torgue Value Correct Torgue Value

#6 Nut 100 N-m/75 ft. lbs. 45 N-m/35 ft. lbs. #9 Bolt 20 N-m/15 ft. lbs. 56 N-m/42 ft. lbs.

Please note the differences in your manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.