HARD TOP HEADER TRIM PLUGS DIFFICULT TO REMOVE (MODIFY). Cadillac Allante 1990

For 1990-2009 cars

# HARD TOP HEADER TRIM PLUGS DIFFICULT TO REMOVE (MODIFY)

#### SUBJECT: HARD TOP HEADER TRIM PLUGS DIFFICULT TO REMOVE (MODIFY PLUGS)

#### MODELS AFFECTED: 1990-1/2 - 1992 ALLANTES

Some 1990-1/2 - 1992 Allantes equipped with a hard top may exhibit a condition where the hard top header trim plugs that cover the latch mechanisms are difficult to remove by hand. To repair this condition modify the plugs using the following service procedure:

1. Remove plugs from hard top.

2. Enlarge the relief slots in the plugs into a "V" shape using side cutters as shown in Figure 1. Enlarge all four relief slots.

3. Install plugs into hard top header and verify ease of removal.

For warranty purposes use Labor Operation T6555 at .2 hour.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.