BATTERY DRAINS UPDATED INFORMATION. Cadillac Allante 1989

For 1990-2009 cars

# BATTERY DRAINS UPDATED INFORMATION

#### SUBJECT: BATTERY DRAINS

#### MODELS AFFECTED: 1987-1992 ALLANTES

This bulletin provides updated information to be added to Service bulletin T-89-38 Group 8. Information contained in bulletin T-89-38 is appropriate for model years 1987-1992.

The diagnosis procedures in bulletin T-89-38 may lead to replacement of the door unlock switch (theft deterrent switch). The R&R procedures for this switch are found in Section 10 of the appropriate Allante Service Information Manual. The door unlock switch, P/N 1639341 is currently available from GMSPO and is used on either door.

For warranty purposes use Labor Operation R2880 at .7 hour when replacing the right door lock switch and R2881 at .7 hour when replacing the left door lock switch.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.