INFORMATION ON FUEL INJECTION HARNESS REPAIR. Cadillac Allante 1993

For 1990-2009 cars

# INFORMATION ON FUEL INJECTION HARNESS REPAIR

#### SUBJECT: INFORMATION ON FUEL INJECTION HARNESS REPAIR

#### VEHICLES AFFECTED: 1993 "E, K AND V" MODELS WITH 4.6L ENGINE (RPO LD8, L37)

Repair of fuel injection wiring that is located under the intake manifold cover on 1993 E, K, and V cars with 4.6L engines is by harness replacement only. The fuel injection wiring harness part number is 12121298

For vehicles repaired under warranty use:

Labour Operation: J5660 Labour Time: .9 Hours (Rail Fuel replace) When replacing the fuel injection wiring harness.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.