SEATBACK RELEASE HANDLE EFFORT TIGHTEN/LOOSEN ADJUSTMENT NUT. Cadillac Allante 1990

For 1990-2009 cars

# SEATBACK RELEASE HANDLE EFFORT TIGHTEN/LOOSEN ADJUSTMENT NUT

#### SUBJECT: SEAT BACK RELEASE HANDLE DIFFICULT TO OPERATE (TIGHTEN OR LOOSEN ADJUSTMENT NUT)

#### VEHICLES AFFECTED: 1987-1992 CADILLAC ALLANTE

Some 1987-1992 Allantes may experience a condition of the seat back release handle being difficult to operate. This condition may be caused by a misadjusted seat release handle.

To repair this condition use the following procedure:

1. Remove the seat back cover. Refer to Section 10-10-3 of the 1991/1992 Allante Service Information Manual.

2. Loosen locknut. Refer to Figure 1.

3. Tighten or loosen adjustment nut to obtain desired release handle effort. Refer to Figure 1.

4. Tighten locknut.

5. Install seat back cover.

For vehicles repaired under warranty use: 0.3 hour.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.