For 1990-2009 cars

### Removal Procedure

1. Remove the relevant front seat. Refer to Seat Replacement in Seats.
2. Remove the carpeting and the insulation. Refer to Front Floor Panel Carpet Replacement in Interior Trim.
3. Remove the rear floor air outlet nut.
4. Remove the rear floor air outlet.

### Installation Procedure

1. Install the rear floor air outlet.
2. Install the rear floor air outlet nut until fully seated and not stripped.
3. Install the carpeting and the insulation. Refer to Front Floor Panel Carpet Replacement in Interior Trim.
4. Install the relevant front seat. Refer to Seat Replacement in Seats.