For 1990-2009 cars

## Clutch Rotor and/or Bearing Install V5 - Conventional Mount

#### Tools Required

• | J 6083 #24 External Snap Ring Pliers

• | J 8092 Driver Handle

• | J 8433-1 Puller Bar

• | J 8433-3 Forcing Screw

• | J 9481-A Bearing Installer

• | J 21352-A Support Block

• | J 33017 Pulley And Bearing Assembly Installer

• | J 33019 Bearing Staking Tool

• | J 33023-A Puller Pilot

• | J 34992 Compressor Holding Fixture

Notice: Do not support the rotor by resting the pulley rim on a flat surface during the bearing installation or the rotor face will be bent.

1. Place the pulley rotor on the J 21352-A in order to fully support the rotor hub during the bearing installation.
2. Align the new bearing with the hub bore.
3. Using the J 9481-A and the J 8092 , drive the bearing into the hub.

The J 9481-A applies force to the outer race of the bearing.

4. Place the J 33019 and the staking pin in the hub bore.
5. Shift the rotor and bearing assembly on the J 21352-A in order to fully support the hub under the location of the staking pin.
6. Use a heavy-duty rubber band (1) in order to hold the stake pin in the guide of the J 33019 .

Important: Do not allow a metal stake to contact the outer face of the bearing in order to prevent distortion of the outer race.

7. Using care in order to prevent injury, strike the staking pin of the J 33019 . Properly position the stake pin in the guide after each impact on the pin.
8. Continue to strike the pin of the J 33019 until a stake, similar to the original stake, is formed down to, but not touching, the bearing.
9. Stake 3 places 120 degrees apart.
10. With the compressor mounted to the J 34992 , position the rotor and bearing assembly on the front head.
11. Position the J 33017 and the J 33023-A directly over the inner race of the bearing.
12. Position the J 8433-1 on the J 33023-A .
13. Assemble the 2 through bolts and the washers of the J 34992 through the slots of the J 8433-1 .
14. Thread the 2 through bolts into the J 34992 .

Ensure that the thread of the through bolts engages the full thickness of the J 34992 .

15. Tighten the J 8433-3 in the J 8433-1 in order to force the pulley rotor and bearing assembly onto the front head of the compressor.
16. If the J 33017 slips off direct, in-line contact with inner face of the bearing, use the following steps:

16.1. | Loosen the J 8433-3 .

16.2. | Realign the J 33017 and the J 33023-A in order to ensure that the installer clears the front head.

17. Install the rotor and bearing assembly retainer ring using the J 6083 .
18. Install the clutch plate and hub assembly. Refer to Compressor Clutch Plate and Hub Assembly Removal (V5 -- Conventional Mount) .