For 1990-2009 cars

1. Install the front timing belt cover.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the front timing belt cover bolts.

Tighten
Tighten the timing belt cover bolts to 8 N·m (71 lb in).

3. Install the power steering pump pulley.
4. Install the power steering pump pulley bolts.

Tighten the power steering pump pulley bolts after the accessory drive belt is installed.

5. Install the water pump pulley.
6. Install the water pump pulley bolts.

Tighten the water pump pulley bolts after the accessory drive belt is installed.