For 1990-2009 cars

### Removal Procedure

1. Slide the sunscreen all the way rearward.
2. Open the glass panel halfway.
3. Remove the brush cover. Refer to Brush Cover Replacement
4. Remove the covers from the right and left side that conceal the bolts for the glass panel adjustment.
5. Remove the bolts from the glass panel for both sides.
6. Loosen the bolts on both sides. These adjustments raise or lower the glass panel.
7. Adjust the front of the glass panel to 0.1 mm (1/32 in) above the top surface of the roof panel
8. Adjust the rear of the glass panel to 0.1 mm (1/32 in) above the top surface.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the bolts to the glass panel for both sides.

Tighten
Tighten the glass panel bolt to 5 N·m (44 lb in).

2. Install the covers to the right and to the left side that conceal the bolts for glass panel adjustment.
3. Install the brush cover. Refer to Brush Cover Replacement .
4. Close the glass panel.
5. Slide the sunscreen closed.