For 1990-2009 cars

### Removal Procedure

1. Open the front side door.
2. Grasp the door upper sealing strip at the upper outer corner and pull downward to expose the window stop bumper.
3. Remove the window up stop screw.
4. Remove the window up stop.

### Installation Procedure

1. Install the stop bumper.
2. Install the stop bumber screw.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Tighten the stop bumper screw.

Tighten
Tighten the window stop bumper screw to 4 N·m (35 lb in).

4. Push the run channel weatherstrip back into place.
5. Close the front side door.