For 1990-2009 cars

### Conditions for Setting the DTC

This DTC sets when the vehicle's battery voltage momentarily goes above 16.0 V.

### Action Taken When the DTC Sets

The detection of leveling output, and the position out-of-range malfunctions are disabled. This is necessary in order to prevent erroneous detection of malfunction conditions due to engine crank or unusual system voltage conditions.

### Conditions for Clearing the DTC

• | The DTC will clear when battery voltage returns to the nominal range.

• | Use a scan tool in order to clear this DTC.

### Diagnostic Aids

• | Inspect the battery system for proper functionality.

• | This DTC does not require the replacing of the automatic level control (ALC) sensor.

• | This DTC will not cause the LEVELING indicator lamp to flash.

• | Ensure that the automatic leveling control sensor is receiving the correct voltage.

• | Ensure that the ALC sensor has a good ground.