For 1990-2009 cars

### Removal Procedure

1. Loosen the fuel filler cap in order to relieve the system pressure.
2. Remove the intake plenum. Refer to Intake Plenum Replacement in Engine Mechanical.
3. Remove the valve bracket mounting bolt.
4. Disconnect the harness connector from the valve.
5. Disconnect the purge line and the vacuum source line from the valve.
6. Remove the purge valve.

### Installation Procedure

1. Connect the purge line and the vacuum source line to the valve.
2. Connect the harness connector.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the valve bracket mounting bolt.

Tighten
Tighten the bolt to 12 N·m (106 lb in)

4. Install the intake plenum. Refer to Intake Plenum Replacement in Engine Mechanical.
5. Tighten the fuel filler cap.