For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle.
2. Remove the tire and wheel assembly. Refer to Wheel Removal in Tires and Wheels.
3. Remove the fender liner plastic retaining clips.
4. Remove the fender liner plastic nuts.
5. Remove the fender liner from the wheelhouse opening.

### Installation Procedure

1. Install the fender liner to the wheelhouse opening.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the fender liner plastic nuts.

Tighten
Tighten the fender liner plastic nuts to 3 N·m (27 lb in).

3. Install the fender liner plastic retaining clips.
4. Install the tire and wheel assembly. Refer to Wheel Installation in Tires and Wheels.
5. Lower the vehicle.