For 1990-2009 cars

### Removal Procedure

1. Pull the rear window run channel weatherstrip halfway down.
2. Remove the rear window stop bumper screw.
3. Remove the rear window stop bumper.

### Installation Procedure

1. Install the rear window stop bumper.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the rear window stop bumper screw.

Tighten
Tighten the rear window stop bumper screw to 4 N·m (35 lb in).

3. Push the rear window run channel weatherstrip into place.