For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Headlights/Daytime Running Lights (DRL) Schematics
1 | Did you perform the Lighting System Diagnostic System Check? | Go to Step 2 | Go to Diagnostic System Check - Lighting Systems
2 | Verify the proper operation of the following lighting systems:

• | The low beam headlamps

• | The twilight sentinel feature

Are these lighting systems operating properly?

Go to Step 3

Go to Diagnostic System Check - Lighting Systems

3 | Test for a short to ground in the headlamps required indicator control circuit. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 5 | Go to Step 4
4 | Replace the instrument cluster. Refer to Instrument Cluster Replacement in Instrument Panel, Gauges and Console. Is the replacement complete? | Go to Step 5 | --
5 |

1. Connect all connectors and components that were disconnected.
2. Verify that the headlamps required indicator operates properly.

Does the headlamps required indicator operate properly?

System OK

Go to Step 2