For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

1. Remove the rear window upper garnish molding.

UseJ 38778 in order to release the clips that retain the rear window upper garnish molding to the roof panel.

2. Bend downward lightly to release the rear window upper garnish molding from the upper quarter trim finish panels.

### Installation Procedure

1. Insert the rear window upper garnish molding:

1.1. | Bend downward slightly

1.2. | Insert one end of the molding at a time to each upper quarter trim finish panel

2. Retain the holes and push in place in order to insert the rear window upper garnish molding clips to the roof panel.